{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["A、B类2025","C类2025","标准器具2025","热动器具2025","实验室器具2025"],"not_rendered":{"defined_names":8,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"A、B类2025","index":0,"n_rows":654,"n_cols":11,"rows_kept":654}
["序号","  仪表位号","设备名称","规格型号","制造厂商","分类","准确度","周期（月）"]
[12,"PT-107-A","1#炉给水压力变送器","0~6MPa","FOXBORO","B",1,36]
[13,"PT-101-A","1#炉锅炉出口主蒸汽管压力变送器","1151GP8E,0~6MPa","ROSEMOUNT","B",1,36]
[35,"PT-119-A","1#炉汽包压力变送器","0~6MPa",null,"B",1,36]
[2,"PI-102-A","1#炉出口主蒸汽管就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[9,"PI-108-A","1#炉给水阀前就地压力表","Y-150  0-6MPa",null,"A",1.6,6]
[22,"PI-120-1A","1#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[23,"PI-120-2A","1#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[32,"PI-103-A","1#炉汽包就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[36,"PI-129-2A","1#炉省煤器出口集箱就地压力表","Y-150  0-4MPa ",null,"A",1.6,6]
[39,"PI-129-3A","1#炉省煤器出口水压就地压力表","Y-150  0-4MPa ",null,"A",1.6,6]
[54,"PI-108B","2#炉给水阀前就地压力表","Y-150  0-6MPa",null,"A",1.6,6]
[71,"PI-120B","2#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[72,"PI-121B","2#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[77,"PI-103B","2#炉汽包就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[83,"PI-122B","2#炉省煤器出口水压就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[98,"PI-108C","3#炉给水阀前就地压力表","Y-150  0-6MPa",null,"A",1.6,6]
[115,"PI-120C","3#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[116,"PI-121C","3#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[121,"PI-103C","3#炉汽包就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[127,"PI-122C","3#炉省煤器出口水压就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[138,"PI-102-D","4#炉出口主蒸汽管就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[144,"PI-108-D","4#炉给水阀前就地压力表","Y-150  0-6MPa",null,"A",1.6,6]
[157,"PI-120-1D","4#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[158,"PI-120-2D","4#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa",null,"A",1.6,6]
[167,"PI-103-D","4#炉汽包就地压力表","Y-150  0-4MPa",null,"A",1.6,6]
[171,"PI-129-2D","4#炉省煤器出口集箱就地压力表","Y-150  0-4MPa ",null,"A",1.6,6]
[174,"PI-129-3D","4#炉省煤器出口水压就地压力表","Y-150  0-4MPa ",null,"A",1.6,6]
[136,"PT-120-B","2#炉主蒸汽母管压力","0~4MPa",null,"B",1,36]
[186,"PT-120-C","3#炉主蒸汽母管压力","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[33,"LT-102-A","1#炉汽包水位差压变送器","1151DP4S  -220~220MMH2O","ROSEMOUNT","B",1,24]
[34,"LT-103-A","1#炉汽包水位差压变送器","1151DP4S  -220~220MMH2O","ROSEMOUNT","B",1,24]
[21,"TE-116-A","1#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂","A","B等",12]
[38,"TE-106-A","1#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=240mm  ￠5","上自仪三厂","A","B等",12]
[69,"TE-112B","2#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂","A","B等",12]
[76,"TE-110B","2#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂","A","B等",12]
[81,"TE-106-2B","2#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=285mm  ￠5 ","上自仪三厂","A","B等",12]
[113,"TE-112C","3#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂","A","B等",12]
[120,"TE-110C","3#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂","A","B等",12]
[125,"TE-106-2C","3#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=260mm  ￠5 ","上自仪三厂","A","B等",12]
[154,"TE-116-D","4#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂","A","B等",12]
[173,"TE-106-D","4#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=270mm  ￠5","上自仪三厂","A","B等",12]
[168,"LT-102-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2..2kPa","ROSEMOUNT","B",1,24]
[169,"LT-103-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2.2kPa","ROSEMOUNT","B",1,24]
[14,"TE-103-A","1#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂","A","B等",12]
[28,"TE-120-A","1#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂","A","B等",12]
[29,"TE-105-A","1#炉排烟温度热电偶","WRN2-330  K  L=1000mm","上自仪三厂","A","B等",12]
[30,"TE-115-A","1#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K  L=325mm  ￠5","上自仪三厂","A","B等",12]
[31,"TE-114-A","1#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂","A","B等",12]
[47,"TE-101-A","1#炉主蒸汽出口温度热电偶","WRN2-13 K L=370mm  ￠5","上自仪三厂","A","B等",12]
[64,"TE-103B","2#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂","A","B等",12]
[92,"TE-120B","2#炉母管前蒸汽温度热电偶","WRE2-625  L=450mm  ￠6","上自仪三厂","A","B等",12]
[90,"TE-101B","2#炉主蒸汽出口温度热电偶","WRN-330 K L=450mm  ￠5 ","上自仪三厂","A","B等",12]
[108,"TE-103C","3#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂","A","B等",12]
[137,"TE-120C","3#炉母管前蒸汽温度热电偶","WRE2-625  L=380mm  ￠6","上自仪三厂","A","B等",12]
[134,"TE-101C","3#炉主蒸汽出口温度热电偶","WRN-330 K  L=545mm  ￠5 ","上自仪三厂","A","B等",12]
[149,"TE-103-D","4#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂","A","B等",12]
[180,"TE-120-D","4#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂","A","B等",12]
[164,"TE-105-D","4#炉排烟温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂","A","B等",12]
[165,"TE-115-D","4#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂","A","B等",12]
[166,"TE-114-D","4#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂","A","B等",12]
[182,"TE-101-D","4#炉主蒸汽出口温度热电偶","WRN2-14HK L=370mm ￠6 0--1000℃","上自仪三厂","A","B等",12]
[122,"LT-102C","3#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT","B",1,24]
[123,"LT-103-C","3#炉汽包水位差压变送器","3051S2CD1A2F12A1AB3M5","ROSEMOUNT","B",1,24]
[78,"LT-102B","2#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT","B",1,24]
[79,"LT-103-B","2#炉汽包水位差压变送器","3051S2CD1A2F12A1AB3M5","ROSEMOUNT","B",1,24]
[74,"PT-104-1B","2#炉炉膛负压1变送器","1151GP3E,-200Pa~+200Pa","ROSEMOUNT","B",1,36]
[75,"PT-104-2B","2#炉炉膛负压2变送器","1151GP3E,-200Pa~+200Pa","ROSEMOUNT","B",1,36]
[76,"LT-102-A","1#炉汽包水位差压变送器","1151DP4S  -220~220MMH2O","ROSEMOUNT","B",{"v":1,"d":"1.0"},24]
[77,"LT-102B","2#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT","B",{"v":1,"d":"1.0"},24]
[78,"LT-102C","3#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT","B",{"v":1,"d":"1.0"},24]
[79,"LT-102-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2..2kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},24]
[80,"LT-103-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2.2kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},24]
[60,"PT-107-1B","2#炉给水压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[61,"PT-107-2B","2#炉给水压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[62,"PT-101-1B","2#炉锅炉出口主蒸汽管压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[63,"PT-101-2B","2#炉锅炉出口主蒸汽管压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[67,"FT-103B","2#炉减温水流量变送器","1151DP4E","ROSEMOUNT","B",1,36]
[80,"PT-119B","2#炉汽包压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[106,"PT-101-1C","3#炉锅炉出口主蒸汽管压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[107,"PT-101-2C","3#炉锅炉出口主蒸汽管压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[135,"FT-101C","3#炉主蒸汽流量变送器","1151DP5E,0~60kPa","ROSEMOUNT","B",1,36]
[111,"FT-103C","3#炉减温水流量变送器","1151DP4E","ROSEMOUNT","B",1,36]
[104,"PT-107-1C","3#炉给水压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[105,"PT-107-2C","3#炉给水压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[91,"FT-101B","2#炉主蒸汽流量变送器","1151DP5E 0~60kPa","ROSEMOUNT","B",1,36]
[118,"PT-104--2C","3#炉炉膛压力变送器","1151GP3E,-200Pa~+200Pa","ROSEMOUNT","B",1,36]
[119,"PT-104--1C","3#炉炉膛压力测量压力变送器","1151GP3E,-200Pa~+200Pa","ROSEMOUNT","B",1,36]
[96,"FT-104C","3#炉风量流量变送器","1151DP,0~1kPa","ROSEMOUNT","B",1,36]
[124,"PT-119C","3#炉汽包压力变送器","1151GP8E,0~4MPa","ROSEMOUNT","B",1,36]
[148,"PT-107-D","4#炉给水压力","0~6MPa",null,"B",1,36]
[170,"PT-119-D","4#炉汽包压力","0~6MPa",null,"B",1,36,"2024-08-28"]
[183,"PT-101-D","4#炉主蒸汽压力","0~6MPa",null,"B",1,36,"2024-08-28"]
{"$rows_empty":100}
[13,"LT-304","2#除氧器水箱水位差压变送器","1151DP4E,-14~0kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[32,"PT-302","加热蒸气母管压力变送器","1151GP6E12M1B3D2","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[36,"PT-309","1#给水泵出口压力变送器","1151GP7E,0~4MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[37,"PT-312","2#给水泵出口压力变送器","1151GP7E,0~4MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[38,"PT-315","3#给水泵出口压力变送器","1151GP7E,0~4MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[39,"PT-316","给水母管压力变送器","1151GP7E,0~4MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[12,"LT-303","1#除氧器水箱水位差压变送器","1151DP4E,-14~0kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[15,"LT-353","3#除氧器水位差压变送器","1151DP4S,-14~0kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[41,"PT-369","4#给水泵出口压力变送器","0~4MPa",null,"B",{"v":1,"d":"1.0"},"检修期 "]
[42,"PT-601","偶合器冷却水母管压力"," ",null,"C",{"v":1,"d":"1.0"},36]
[14,"LT-305","疏水箱水位压力变送器","1151,0~30kpa","ROSEMOUNT","C",{"v":1,"d":"1.0"},36]
[1,"FT-301","凝结水回水流量","1151,0~25kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},36]
[33,"PT-303","1#除氧器压力变送器","0~30kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},"检修期"]
[35,"PT-305","2#除氧器压力变送器","0~30kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},"检修期 "]
[40,"PT-353","3#除氧器压力变送器","0~90kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},"检修期 "]
[2,"FT-302","除氧器蒸汽母管出口流量"," ",null,"C"]
[3,"FT-353","除养器加热蒸汽流量","电磁流量计",null,"C"]
[4,"JY-PI-01","1#加药计量泵出口压力表",null,null,"C"]
[5,"JY-PI-02","2#加药计量泵出口压力表",null,null,"C"]
[6,"JY-PI-03","3#加药计量泵出口压力表",null,null,"C"]
[7,"JY-PI-04","4#加药计量泵出口压力表",null,null,"C"]
[8,"JY-PI-05","5#加药计量泵出口压力表",null,null,"C"]
[9,"LS-306","1#工业水箱水位浮球液位控制器","UQK-01",null,"C"]
[10,"LS-307","2#工业水箱水位浮球液位控制器","UQK-01",null,"C"]
[11,"LT-301","1#除氧器水箱水位磁助式液位计","UHZ-5110",null,"C"]
[17,"PI-304","1#除氧器就地压力表","Y-150  0~0.1MPa",null,"C"]
[18,"PI-306","2#除氧器就地压力表","Y-150  0-0.1MPa",null,"C"]
[19,"PI-307","1#给水泵进口就地压力表","Y-150  0-0.4MPa",null,"C"]
[20,"PI-308","1#给水泵出口就地压力表","Y-150  0~6MPa",null,"C"]
[21,"PI-310","2#给水泵进口就地压力表","Y-150  0~0.6MPa",null,"C"]
[22,"PI-311","2#给水泵出口就地压力表","Y-150  0~6MPa",null,"C"]
[23,"PI-313","3#给水泵进口就地压力表","Y-150  0~0.6MPa",null,"C"]
[24,"PI-314","3#给水泵出口就地压力表","Y-150  0~6MPa",null,"C"]
[25,"PI-317","给水母管就地压力表","Y-150  0~6MPa",null,"C"]
[26,"PI-318","4#给水泵进口就地压力表","Y-150  0~0.4MPa",null,"C"]
[27,"PI-319","4#给水泵出口就地压力表","0~6MPa",null,"C"]
[28,"PI-320","连续排污扩容器就地压力表","Y-150  0~1.6MPa",null,"C"]
[29,"PI-351","工业水泵出口压力弹簧管压力表","Y-150  0~1MPa  1.5级",null,"C"]
[30,"PI-352","疏水泵出口压力弹簧管压力表","Y-150  0~1MPa  1.5级",null,"C"]
[31,"PI-354","3#除氧器压力弹簧管压力表","Y-150  0~0.1MPa  1.5级",null,"C"]
[34,"PT-303A","1#除氧器压力变送器","1151GP4E,0~30kPa迁-12kPa",null,"C"]
[43,"TE-302","1#除氧器水箱温度热电阻","WZP-231(K),Pt100",null,"C"]
[44,"TE-304","2#除氧器水箱温度","WZP-231(K),Pt100",null,"C"]
[45,"TE-352","3#除氧器水箱温度","WZP-231(K),Pt100",null,"C"]
[46,"TE-352","3#除氧器水箱双只热电阻","WZP2-231 PT100 650X500MM   M27X2",null,"C"]
[47,"TI-305 ","1#除氧器压力式温度计","WTQ-280   0~200℃",null,"C"]
[48,"TI-306","2#除氧器压力式温度计","WTQ-280   0~200℃",null,"C"]
[49,"TI-351","3#除氧器水箱双金属温度计","WSS-581W  0~150℃  L=1000MM d=10MM  M27X2",null,"C"]
[50,"XZQY-35-BH-1","1#饱和蒸汽温度表","WSS-301/0~100℃/轴向",null,"C"]
[51,"XZQY-35-BH-2","2#饱和蒸汽温度表","WSS-301/0~100℃/轴向",null,"C"]
[52,"XZQY-35-BH-3","3#饱和蒸汽温度表","WSS-301/0~100℃/轴向",null,"C"]
[53,"XZQY-35-BH-4","4#饱和蒸汽温度表","WSS-301/0~100℃/轴向",null,"C"]
[54,"XZQY-35-GR-1","1#过热蒸汽温度表","WSS-301 0~100℃/轴向",null,"C"]
[55,"XZQY-35-GR-2","2#过热蒸汽温度表","WSS-301 0~100℃/轴向",null,"C"]
[56,"XZQY-35-GR-3","3#过热蒸汽温度表","WSS-301 0~100℃/轴向",null,"C"]
[57,"XZQY-35-GR-4","4#过热蒸汽温度表","WSS-301 0~100℃/轴向",null,"C"]
[58,"XZQY-35-LS-1","1#炉水温度表","WSS-301 0~100℃/轴向",null,"C"]
[59,"XZQY-35-LS-2","2#炉水温度表","WSS-301 0~100℃/轴向",null,"C"]
[60,"XZQY-35-LS-3","3#炉水温度表","WSS-301 0~100℃/轴向",null,"C"]
[61,"XZQY-35-LS-4","4#炉水温度表","WSS-301 0~100℃/轴向",null,"C"]
[62,"PT-601","吸热器进汽压力变送器","3051STG2A2B21AB4M5，0~1MPa","ROSEMOUNT","C"]
[63,"PI-601","吸热器进汽压力表","0~1.0MPa","WIKA","C"]
[64,"PI-603","吸热器出水热泵出口压力表","0~1.0MPa","WIKA","C"]
[65,"LT-601","吸热器磁翻板液位计","KTLHZ-6525，1.6M","安徽天康","C"]
[66,"TE-601","吸热器温度热电阻","PT100",null,"C"]
[93,"PT-115C","3#炉除尘器后烟气负压压力变送器","1151GP3E,-3500Pa~0Pa","ROSEMOUNT","C",1]
[112,"PT-113C","3#炉空气预热器出口风压压力变送器","1151GP4E,0~7kPa","ROSEMOUNT","C",1]
[128,"PT-106C","3#炉省煤器后烟气负压压力变送器","1151GP3E,-800Pa~0Pa","ROSEMOUNT","C",1]
[133,"PT-112C","3#炉送风机出口风压压力变送器","1151GP4E,0~8kPa","ROSEMOUNT","C",1]
[139,"PT-115-D","4#炉除尘器后烟气压力","-8000Pa~0Pa",null,"C",1]
[140,"PT-127-D","4#炉除尘器入口烟气压力(右)","-7000Pa~0Pa",null,"C",1]
[141,"PT-128-D","4#炉除尘器入口烟气压力(左)","-7000Pa~0Pa",null,"C",1]
[162,"PT-113-D","4#炉炉膛入口风压(右)","0~5000Pa",null,"C",1]
[163,"PT-116-D","4#炉炉膛入口风压(左)","0~5000Pa",null,"C",1]
[179,"PT-112-D","4#炉送风机出口风压","0~6000Pa",null,"C",1]
[159,"PT-104-D","4#炉炉膛负压1","-200Pa~200Pa",null,"C",1]
[160,"PT-110-D","4#炉炉膛负压2","-200Pa~200Pa",null,"C",1]
[175,"PT-105-D","4#炉省煤器前烟气负压压力变送器","-8000Pa~0Pa",null,"C",1]
[177,"FT-104-D","4#炉送风风量","1151DP3S52M1B32, 0~1kPa","ROSEMOUNT","C",1]
[20,"PI-122-A","1#炉空气预热器出口风压压力就地压力表左","Y-150  0~600Pa",null,"C"," "," "]
[195,"AT-101A","1#锅炉炉膛出口氧量分析仪","ZO-4（三）","上海可贵离子导体公司","B",null,3]
[196,"AT-101B","2#锅炉炉膛出口氧量分析仪","ZO-4（三）","上海可贵离子导体公司","B",null,3]
[197,"AT-101C","3#锅炉炉膛出口氧量分析仪","ZO-4（三）","上海可贵离子导体公司","B",null,3]
[198,"AT-101D","4#锅炉炉膛出口氧量分析仪","ZO-4（三）","上海可贵离子导体公司","B",null,3]
[25,"PT-551","5#减温减压器出口压力变送器","0-2MPa","FOXBORO","B",{"v":1,"d":"1.0"},36]
[2,"FT-502","2#热用户流量差压变送器","1151DP4E 0~13.5kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[21,"PT-513","3#减温减压器二次压力变送器","1151GP7E,0~1.3MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[20,"PT-512","2#减温减压器二次压力变送器","1151GP7E,0~1.3MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[19,"PT-511","1#减温减压器二次压力变送器","1151GP7E,0~1.3MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[22,"PT-514","4#减温减压器二次压力变送器","1151GP7E,0~0.5MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[23,"PT-515","一次蒸汽压力变送器","1151GP6E,0~0.49MPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[3,"PI-118","主蒸汽母管就地压力表","Y-150  0~4MPa"," ","A",1.6,12]
[4,"PI-504","一次蒸汽就地压力表","Y-150  0~4MPa",null,"A"," ",12]
[11,"PI-513","1#减温减压器出口就地压力表","Y-100  0~2.5MPa",null,"A"," ",12]
[12,"PI-514","2#减温减压器出口就地压力表","Y-100  0~2.5MPa",null,"A"," ",12]
[13,"PI-515","3#减温减压器出口就地压力表","Y-100  0~2.5MPa",null,"A"," ",12]
[14,"PI-516","4#减温减压器出口就地压力表","Y-100  0~1.6MPa",null,"A"," ",12]
[129,"PI-444","化水空气储罐压力","0-1.6MPa","WIKA","A",1.6,6]
[133,"PT-421","空气储罐压力","0~1MPa","FOXBORO","B",{"v":1,"d":"1.0"},36]
[32,"FT-406","至锅炉除盐水流量","1151DP5E 0-80kPa",null,"B",{"v":1,"d":"1.0"},36]
[34,"FT-408","碱喷射器出口流量","1151DP4J  0-25kPa",null,"B",{"v":1,"d":"1.0"},36]
[33,"FT-407","酸喷射器出口流量","1151DP4J  0-25kPa",null,"B",{"v":1,"d":"1.0"},36]
[14,"314-PT-02","消防水进水总管压力变送器","1151GP4E","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[132,"PT-408","除盐水总管压力","1151GPS12I5","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[134,"PT-422","软化水总管压力","1151GPS12I5","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[16,"APO4T-1","磷酸根分析仪",5000,"HACH","B",null,1]
[17,"ASIT-1 ","阴床出水硅酸根分析仪","HK118W","北京华科仪","B",null,1]
[81,"PH-12","1、2#炉水PH计","8362SC","HACH","B",null,6]
[83,"PH-34","3、4#炉水PH计","8362SC","HACH","B",null,6]
[1,"WIT","地磅秤","SCS-100","中美合资攀枝花托利多电子衡器有限公司","A","III",12]
[1,"WIT  ","1801541","食堂电子台秤","TCS-500kg","惠州市英衡电子科技有限公司","B","III"]
[57,"CEMS-1","烟气在线监测系统","SMC-9021","SICK","B",null,"每周"]
[58,"210-PI-026","膜制氮装置空气储罐出口压力","0~1.6MPa","WIKA","A",1.6,6]
[67,"210-PI-053","吸附制氮机1#塔压力","0~1.6MPa","WIKA","A",1.6,6]
[68,"210-PI-054","吸附制氮机2#塔压力","0~1.6MPa","WIKA","A",1.6,6]
[71,"210-PI-048","吸附制氮机储罐压力","0~1.6MPa","WIKA","A",1.6,6]
[72,"210-PI-046","吸附制氮机缓冲罐压力","0~1.6MPa","WIKA","A",1.6,6]
[84,"210-PI-GL1","4#空压机3#过滤器进口压力","0~1.6MPa","WIKA","A",1.6,6]
[85,"210-PI-GL2","4#空压机3#过滤器出口压力","0~1.6MPa","WIKA","A",1.6,6]
[92,"210-PI-GL11","小空压机1#过滤器进口压力","0~1.6MPa","WIKA","A",1.6,6]
[93,"210-PI-GL22","小空压机1#过滤器出口压力","0~1.6MPa","WIKA","A",1.6,6]
[98,"210-PI-1","3#空压机2#过滤器进口压力","0~1.6MPa","WIKA","A",1.6,6]
[99,"210-PI-2","3#空压机2#过滤器出口压力","0~1.6MPa","WIKA","A",1.6,6]
[102,"210-PI-1A","1#外加热再生干燥器A塔压力","0~1.6MPa","WIKA","A",1.6,6]
[103,"210-PI-1B","1#外加热再生干燥器B塔压力","0~1.6MPa","WIKA","A",1.6,6]
[104,"210-PI-2A","2#外加热再生干燥器A塔压力","0~1.6MPa","WIKA","A",1.6,6]
[105,"210-PI-2B","2#外加热再生干燥器B塔压力","0~1.6MPa","WIKA","A",1.6,6]
[116,"210-PI-G3","3#冷干机油过滤器压力","0~1.6MPa","WIKA","A",1.6,6]
[119,"210-PI-052D","3#PS过滤器出口压力","0~1.6MPa","WIKA","A",1.6,6]
[120,"210-PI-052B","3#干燥器B塔压力","0~1.6MPa","WIKA","A",1.6,6]
[121,"210-PI-052A","3#干燥器A塔压力","0~1.6MPa","WIKA","A",1.6,6]
[122,"210-PI-052C","3#CS过滤器压力","0~1.6MPa","WIKA","A",1.6,6]
[129,"210-PI-MS3","4#冷干机MS3油过滤器压力","0~1.6MPa","WIKA","A",1.6,6]
[132,"210-PI-053D","4#PS过滤器出口压力","0~1.6MPa","WIKA","A",1.6,6]
[133,"210-PI-053B","4#干燥器B塔压力","0~1.6MPa","WIKA","A",1.6,6]
[134,"210-PI-053A","4#干燥器A塔压力","0~1.6MPa","WIKA","A",1.6,6]
[135,"210-PI-053C","4#CS过滤器压力","0~1.6MPa","WIKA","A",1.6,6]
[142,"210-PI-121","2#缓冲罐压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[143,"210-PI-120","1#缓冲罐压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[144,"210-PI-123","4#缓冲罐压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[145,"210-PI-122","3#缓冲罐压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[146,"210-PI-124","6#缓冲罐压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[147,"210-PI-125","5#缓冲罐压缩空气压力（供界外）","0~1.6MPa","WIKA","A",1.6,6]
[150,"210-PI-063B","2#氮气储罐压力","0~1.6MPa","WIKA","A",1.6,6]
[153,"210-PI-062","卷曲机压缩空气压力","0~1.6MPa","WIKA","A",1.6,6]
[225,"210-PI-061A","1#空气储罐压力","0~1.6MPa","WIKA","A",1.6,6]
[227,"210-PI-061B","2#空气储罐压力","0~1.6MPa","WIKA","A",1.6,6]
[228,"210-PI-063A","1#氮气储罐压力","0~1.6MPa","WIKA","A",1.6,6]
[140,"210-PT-118","氮气储罐压力","821GM-1S1SM2-AM ","FOXBORO","B",{"v":1,"d":"1.0"},36]
[169,"312-FT-02","丝束冷却水出水总管流量","1151DP5E12M1B3D2  0~60kPa","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[52,"210-PT-202","冷冻水出水总管压力","IGP20-T22D21F-M1L1 0~0.8MPa","FOXBORO公司","B",{"v":1,"d":"1.0"},36]
[365,"WIT  ","08-0302","1#成品秤","SCS-1","托利多        ","A","III",12]
[366,"WIT  ","08-0303","2#成品秤","SCS-1","托利多        ","A","III",12]
[80,"PT","06-2211","卷曲机压缩空气总管压力变送器","3051S1TG2A2E11A1AB4D1I5M504","ROSEMOUNT","B",{"v":1,"d":"1.0"},36]
[44,"PT","06-0313","VLA总管压力变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","B",{"v":1,"d":"1.0"},12]
[45,"PT","06-2313","VLA总管压力变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","B",{"v":1,"d":"1.0"},12]
[90,"PI   ","04-0413","脏丙酮储槽压力表 ","0~1.0MPa","WIKA","A",1.6,6]
[144,"PI   ","04-460","丙酮蒸发炉冷凝器压力表 ","0~1.0MPa","WIKA","A",1.6,6]
[21,"PI   ","04-0102","1#未过滤浆液贮槽压力压力表      ","Y100  0~0.25MPa","北京布莱迪","A",1.6,6]
[22,"PI   ","04-0103","2#未过滤浆液贮槽压力压力表     ","Y100  0~0.25MPa","北京布莱迪","A",1.6,6]
[49,"PI   ","04-0206","二级过滤浆液贮槽压力压力表     ","Y100  0~0.25MPa","北京布莱迪","A",1.6,6]
[77,"PI   ","04-0316","3#未过滤浆液贮槽压力压力表      ","Y100  0~0.25MPa","北京布莱迪","A",1.6,6]
[62,"PI","10-0268","1#集液槽压力表","0~1.0MPa","WIKA","A",1.6,6]
[229,"PI","10-2268","2#集液槽压力表","0~1.0MPa","WIKA","A",1.6,6]
[289,"PI","17-0308","氮气吹气缓冲槽压力表","0~1.0MPa","WIKA","A",1.6,6]
[2,"PT","10-0003","VLA总管压力变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","B",{"v":1,"d":"1.0"},12]
[9,"PT","10-0033","冷却水总管压力变送器","3051S1T08A2E11A1AB4D115M5","ROSEMOUNT","B",{"v":1,"d":"1.0"},12]
[1,"TTE/MTE","-11-014-","01",1,"制浆二层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[2,"TTE/MTE","-11-017-","01",1,"一期纺丝一层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[3,"TTE/MTE","-11-018-","01",1,"一期纺丝二层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[4,"TTE/MTE","-11-036-","01",1,"喷丝帽清洗间温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[5,"TTE/MTE","-11-040-","01",1,"中控室温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[6,"TTE/MTE","-11-233-","01",1,"化验室温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[7,"TTE/MTE","-11-233-","02",2,"化验室精密仪器间温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[8,"TTE/MTE","-11-237-","01",1,"喷丝帽组装无尘间温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[9,"TTE/MTE","-11-240-","01",1,"卷曲机检修间温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[10,"TTE/MTE","-11-252-","01",1,"物检室温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[11,"TTE/MTE","-11-214-","01",1,"制浆一层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[12,"TMT","-04-15",null,null,"溶解釜区域温湿度变送器","HMT360","VAISALA","B","1℃/3％",24]
[13,"TTE/MTE","-11-217-","01",1,"二期纺丝一层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[14,"TTE/MTE","-11-218-","01",1,"二期纺丝二层温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[15,"TTE/MTE","-11-221-","01",1,"二期干燥卷曲区温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[16,"TTE/MTE","-11-223-","01",1,"二期摆丝一层温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[17,"TTE/MTE","-11-223-","02",2,"二期摆丝二层温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[18,"TTE/MTE","-11-021-","01",1,"一期干燥卷曲区温湿度变送器","HMP363A22BCF1B4BC2A1A4","VAISALA","B","1℃/2％",24]
[19,"TTE/MTE","-11-023-","01",1,"一期摆丝一层温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[20,"TTE/MTE","-11-023-","02",2,"一期摆丝二层温湿度变送器","HMP231A2A0A2AA12A1A3B","VAISALA","B","1℃/2％",24]
[26,"AE","-11-014-","空调气体测试仪","01","制浆空调丙酮分析仪","PIRECL","DET-TRONICS","B","±1.0%","1周"]
[27,"AE","-11-017-","空调气体测试仪","01","纺丝空调丙酮分析仪","PIRECL","DET-TRONICS","B","±1.0%","2周"]
[28,"AE","-11-021-","空调气体测试仪","01","干燥机空调丙酮分析仪","PIRECL","DET-TRONICS","B","±1.0%","3周"]
[1,"AT-1001","A-2与A-3压滤机顶紧螺杆一端中间立柱靠A泵一侧丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[2,"AT-1002","A-5与A-6压滤机顶紧螺杆一端中间立柱靠A泵一侧丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[3,"AT-1003","A-8与A-9压滤机顶紧螺杆一端中间立柱靠A泵一侧丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[4,"AT-1004","A-12与A-13压滤机靠阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[5,"AT-1005","A-15与A-16压滤机靠阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[6,"AT-1006","A-18与A-19压滤机靠阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[7,"AT-1007","A-22与A-23压滤机中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[8,"AT-1008","A-28与A-29压滤机靠阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[9,"AT-1009","A-33与A-34压滤机靠顶紧螺杆端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[10,"AT-1010","A-38与A-39压滤机阀门端中间墙面上丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[11,"AT-1011","M2泵与M3泵中间位置丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[12,"AT-1012","1#R釜与2#R釜搅拌轴中间位置丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[13,"AT-1013","R釜出料泵中间位置丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[14,"AT-1014","2B#釜出料泵旁丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[15,"AT-1015","C-2泵对面墙面上丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[16,"AT-1016","S-3泵对面墙面上丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[17,"AT-1017","C-8与C-9压滤机阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[18,"AT-1018","S-8与S-9压滤机阀门端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[19,"AT-1019","C-3与C-4压滤机顶紧螺杆一端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[20,"AT-1020","S-3与S-4压滤机顶紧螺杆一端中间立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[21,"AT-1021","制浆一楼蒸发炉旁边楼梯口立柱内侧丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[22,"AT-1022","丙酮区回流槽围堰中间丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[23,"AT-1023","稀丙酮槽围堰中间靠进稀丙酮泵丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[24,"AT-1024","丙酮槽车卸料站洗眼站一侧消防箱旁立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[25,"AT-1025","界外丙酮储槽丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[26,"AT-1026","1#-4#丙酮储槽丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[27,"AT-1027","5#-6#丙酮储槽丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[28,"AT-2001","纺丝一楼纺丝机1A面墙面1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[29,"AT-2002","纺丝一楼纺丝机1A面墙面2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[30,"AT-2003","纺丝一楼纺丝机1B与2A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[31,"AT-2004","纺丝一楼纺丝机1B与2A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[32,"AT-2005","纺丝一楼纺丝机2B与3A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[33,"AT-2006","纺丝一楼纺丝机2B与3A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[34,"AT-2007","纺丝一楼纺丝机3B与4A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[35,"AT-2008","纺丝一楼纺丝机3B与4A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[36,"AT-2009","纺丝一楼纺丝机4B面墙面1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[37,"AT-2010","纺丝一楼纺丝机4B面墙面2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[38,"AT-2011","纺丝一楼纺丝机1A面与卷曲机之间墙面丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[39,"AT-2012","纺丝一楼一期与二期之间卷曲机前立柱丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[40,"AT-2013","纺丝一楼纺丝机4B面与卷曲机之间墙面丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[41,"AT-2014","一期干燥机中间尾部墙面丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[42,"AT-2015","二期干燥机中间尾部墙面丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[43,"AT-2016","喷丝帽清洗间中部丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[44,"AT-2017","纺丝二楼纺丝机1A面墙面1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[45,"AT-2018","纺丝二楼纺丝机1A面墙面2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[46,"AT-2019","纺丝二楼纺丝机1B与2A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[47,"AT-2020","纺丝二楼纺丝机1B与2A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[48,"AT-2021","纺丝二楼纺丝机2B与3A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[49,"AT-2022","纺丝二楼纺丝机2B与3A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[50,"AT-2023","纺丝二楼纺丝机3B与4A面之间立柱1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[51,"AT-2024","纺丝二楼纺丝机3B与4A面之间立柱2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[52,"AT-2025","纺丝二楼纺丝机4B面墙面1#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[53,"AT-2026","纺丝二楼纺丝机4B面墙面2#丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[54,"AT-3001","集水井硫化氢浓度检测仪","NTMSN10W（传感器）+UD10A5N25W2N(变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[55,"AT-3002","冷水机车间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[56,"AT-3003","制氮机车间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[57,"AT-4001","危险品库氢气浓度检测仪","GTSH21000PC(传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[58,"AT-4002","危险品库乙炔气浓度检测仪","CGS（传感器）+UD10A5N25W2C（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[59,"AT-5001","信息中心机房氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[60,"AT-5002","总降七氟丙烷气瓶间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[61,"AT-5003","丝束七氟丙烷气瓶间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[62,"AT-5004","丝束二氧化碳气瓶间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[63,"AT-3005","集水井氧气度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[64,"AT-3006","危险品库氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[65,"AT-5006","喷丝帽清洗间氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[66,"AT-5005","丝束中控室氧气浓度检测仪","GTSO225VT（传感器）+UD10A5N25T2（变送器）","DET-TRONICS ",{"$nulls":3},"B",1,12]
[67,"AT-1028","丙酮贮槽氮封氧含量分析小屋丙酮浓度检测仪","PIRECLA1D1Y1","DET-TRONICS ",{"$nulls":3},"B",1,12]
[1,"PI-102-A","1#炉出口主蒸汽管就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[2,"PI-108-A","1#炉给水阀前就地压力表","Y-150  0-6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[3,"PI-120-1A","1#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[4,"PI-120-2A","1#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[5,"PI-103-A","1#炉汽包就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[6,"PI-129-2A","1#炉省煤器出口集箱就地压力表","Y-150  0-4MPa ","WIKA",{"$nulls":3},"A",1.6,6]
[7,"PI-129-3A","1#炉省煤器出口水压就地压力表","Y-150  0-4MPa ","WIKA",{"$nulls":3},"A",1.6,6]
[8,"PI-108B","2#炉给水阀前就地压力表","Y-150  0-6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[9,"PI-120B","2#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[10,"PI-121B","2#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[11,"PI-103B","2#炉汽包就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[12,"PI-122B","2#炉省煤器出口水压就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[13,"PI-108C","3#炉给水阀前就地压力表","Y-150  0-6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[14,"PI-120C","3#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[15,"PI-121C","3#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[16,"PI-103C","3#炉汽包就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[17,"PI-122C","3#炉省煤器出口水压就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[18,"PI-102-D","4#炉出口主蒸汽管就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[19,"PI-108-D","4#炉给水阀前就地压力表","Y-150  0-6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[20,"PI-120-1D","4#炉炉前锅筒蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[21,"PI-120-2D","4#炉炉前集箱出口蒸汽就地压力表","Y-250  0-4MPa","青岛四方",{"$nulls":3},"A",1.6,6]
[22,"PI-103-D","4#炉汽包就地压力表","Y-150  0-4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[23,"PI-129-2D","4#炉省煤器出口集箱就地压力表","Y-150  0-4MPa ","WIKA",{"$nulls":3},"A",1.6,6]
[24,"PI-129-3D","4#炉省煤器出口水压就地压力表","Y-150  0-4MPa ","WIKA",{"$nulls":3},"A",1.6,6]
[25,"TE-103-A","1#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[26,"TE-120-A","1#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[27,"TE-105-A","1#炉排烟温度热电偶","WRN2-330  K  L=1000mm","上自仪三厂",{"$nulls":3},"A","B等",12]
[28,"TE-115-A","1#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K  L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[29,"TE-114-A","1#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[30,"TE-101-A","1#炉主蒸汽出口温度热电偶","WRN2-13 K L=370mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[31,"TE-103B","2#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[32,"TE-120B","2#炉母管前蒸汽温度热电偶","WRE2-625  L=380mm  ￠6","上自仪三厂",{"$nulls":3},"A","B等",12]
[33,"TE-101B","2#炉主蒸汽出口温度热电偶","WRN-330 K L=545mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[34,"TE-103C","3#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[35,"TE-120C","3#炉母管前蒸汽温度热电偶","WRE2-625  L=380mm  ￠6","上自仪三厂",{"$nulls":3},"A","B等",12]
[36,"TE-101C","3#炉主蒸汽出口温度热电偶","WRN-330 K  L=545mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[37,"TE-103-D","4#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[38,"TE-120-D","4#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[39,"TE-105-D","4#炉排烟温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[40,"TE-115-D","4#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[41,"TE-114-D","4#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[42,"TE-101-D","4#炉主蒸汽出口温度热电偶","WRN2-13 K L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[43,"TE-116-A","1#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[44,"TE-106-A","1#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=240mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[45,"TE-112B","2#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[46,"TE-110B","2#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[47,"TE-106-2B","2#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=285mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[48,"TE-112C","3#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[49,"TE-110C","3#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[50,"TE-106-2C","3#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=260mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[51,"TE-116-D","4#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[52,"TE-106-D","4#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=270mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[53,"PI-444","化水空气储罐压力","Y-100  0-1MPa","WIKA",{"$nulls":3},"A",1.6,6]
[54,"210-PI-026","膜制氮装置空气储罐出口压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[55,"210-PI-053","吸附制氮机1#塔压力","0~1kg/cm2   0~160PSI","ASHCROFT",{"$nulls":3},"A",1.6,6]
[56,"210-PI-054","吸附制氮机2#塔压力","0~1kg/cm2   0~160PSI","ASHCROFT",{"$nulls":3},"A",1.6,6]
[57,"210-PI-048","吸附制氮机储罐压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[58,"210-PI-046","吸附制氮机缓冲罐压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[59,"210-PI-GL1","1#油过滤器进口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[60,"210-PI-GL2","1#油过滤器出口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[61,"210-PI-GL11","一级过滤器进口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[62,"210-PI-GL22","一级过滤器出口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[63,"210-PI-1","3#OS过滤器出口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[64,"210-PI-2","3#除油器进口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[65,"210-PI-1A","1#外加热再生干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[66,"210-PI-1B","1#外加热再生干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[67,"210-PI-2A","2#外加热再生干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[68,"210-PI-2B","2#外加热再生干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[69,"210-PI-G3","3#冷干机油过滤器压力","0~1.6MPa","上海仪表四厂",{"$nulls":3},"A",1.6,6]
[70,"210-PI-052D","3#PS过滤器出口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[71,"210-PI-052B","3#干燥器B塔压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[72,"210-PI-052A","3#干燥器A塔压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[73,"210-PI-052C","3#CS过滤器压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[74,"210-PI-MS3","4#冷干机MS3油过滤器压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[75,"210-PI-053D","4#PS过滤器出口压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[76,"210-PI-053B","4#干燥器B塔压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[77,"210-PI-053A","4#干燥器A塔压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[78,"210-PI-053C","4#CS过滤器压力","0~1.6MPa","宜昌仪表厂",{"$nulls":3},"A",1.6,6]
[79,"210-PI-121","2#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[80,"210-PI-120","1#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[81,"210-PI-123","4#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[82,"210-PI-122","3#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[83,"210-PI-124","6#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[84,"210-PI-125","5#缓冲罐压缩空气压力（供界外）","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[85,"210-PI-063B","2#氮气储罐压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[86,"210-PI-062","卷曲机压缩空气压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[87,"210-PI-061A","1#空气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[88,"210-PI-061B","2#空气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[89,"210-PI-063A","1#氮气储罐压力","0~1.0MPa","WIKA",{"$nulls":3},"A",1.6,6]
[1,"LT-102-A","1#炉汽包水位差压变送器","1151DP4S  -220~220MMH2O","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},24]
[2,"LT-102B","2#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},24]
[3,"LT-102C","3#炉汽包水位差压变送器","1151DP3E12M1B32, -220~220MMH20","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},24]
[4,"LT-102-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2..2kPa","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},24]
[5,"LT-103-D","4#炉汽包水位差压变送器","1151DP3S52M1B32, -2.2~2.2kPa","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},24]
[6,"PT-06-0313","VLA总管压力变送器","1151DP4S12I5","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},12]
[7,"PT-06-2313","VLA总管压力变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},12]
[8,"PT-10-0003","VLA总管压力变送器","1151DP3S22I5","ROSEMOUNT",{"$nulls":3},"B",{"v":1,"d":"1.0"},12]
[1,"TE-103-A","1#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[2,"TE-116-A","1#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[3,"TE-120-A","1#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[4,"TE-105-A","1#炉排烟温度热电偶","WRN2-330  K  L=1000mm","上自仪三厂",{"$nulls":3},"A","B等",12]
[5,"TE-115-A","1#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K  L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[6,"TE-114-A","1#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[7,"TE-106-A","1#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=240mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[8,"TE-101-A","1#炉主蒸汽出口温度热电偶","WRN2-13 K L=370mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[9,"TE-103B","2#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[10,"TE-112B","2#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[11,"TE-120B","2#炉母管前蒸汽温度热电偶","WRE2-625  L=450mm  ￠6","上自仪三厂",{"$nulls":3},"A","B等",12]
[12,"TE-110B","2#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[13,"TE-106-2B","2#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=285mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[14,"TE-101B","2#炉主蒸汽出口温度热电偶","WRN-330 K L=545mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[15,"TE-103C","3#炉过热器入口温度热电偶","WRN-330 K  L=1000mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[16,"TE-112C","3#炉空气预热器出口温度热电阻","WZP-231 Pt100  L=430mm ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[17,"TE-120C","3#炉母管前蒸汽温度热电偶","WRE2-625  L=380mm  ￠6","上自仪三厂",{"$nulls":3},"A","B等",12]
[18,"TE-110C","3#炉排烟温度热电阻","WZP-330 Pt100   L=900mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[19,"TE-106-2C","3#炉省煤器出口水管温度热电阻","WZP-630 Pt100   L=260mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[20,"TE-101C","3#炉主蒸汽出口温度热电偶","WRN-330 K  L=545mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[21,"TE-103-D","4#炉过热器入口温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[22,"TE-116-D","4#炉空气预热器出口温度热电阻","WZP2-231 Pt100  L=460mm  ￠5 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[23,"TE-120-D","4#炉母管前蒸汽温度热电偶","WRN2-13 K  L=355mm  ￠5  ","上自仪三厂",{"$nulls":3},"A","B等",12]
[24,"TE-105-D","4#炉排烟温度热电偶","WRN2-330  K  L=1000mm  ￠6 ","上自仪三厂",{"$nulls":3},"A","B等",12]
[25,"TE-115-D","4#炉喷水减温器出口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[26,"TE-114-D","4#炉喷水减温器入口蒸汽温度热电偶","WRN2-13 K   L=325mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[27,"TE-106-D","4#炉省煤器出口水温度热电阻","WZP2-231 PT100 L=270mm  ￠5","上自仪三厂",{"$nulls":3},"A","B等",12]
[28,"TE-101-D","4#炉主蒸汽出口温度热电偶","WRN2-14HK L=370mm ￠6 0--1000℃","上自仪三厂",{"$nulls":3},"A","B等",12]
[1,"PI","10-0268","1#集液槽压力表","0~1.0MPa","WIKA",null,null,"A",1.6,6]
[2,"PI","10-2268","2#集液槽压力表","0~1.0MPa","WIKA",null,null,"A",1.6,6]
[4,"PI","04-0413","脏丙酮储槽压力表 ","0~1.0MPa","WIKA",null,null,"A",1.6,6]
[1,"PI-444","化水空气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[2,"PI-102-A","1#炉出口主蒸汽管就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[3,"PI-108-A","1#炉给水阀前就地压力表","0~6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[4,"PI-120-1A","1#炉炉前锅筒蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[5,"PI-120-2A","1#炉炉前集箱出口蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[6,"PI-103-A","1#炉汽包就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[7,"PI-129-2A","1#炉省煤器出口集箱就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[8,"PI-129-3A","1#炉省煤器出口水压就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[9,"PI-108B","2#炉给水阀前就地压力表","0~6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[10,"PI-120B","2#炉炉前锅筒蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[11,"PI-121B","2#炉炉前集箱出口蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[12,"PI-103B","2#炉汽包就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[13,"PI-122B","2#炉省煤器出口水压就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[14,"PI-108C","3#炉给水阀前就地压力表","0~6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[15,"PI-120C","3#炉炉前锅筒蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[16,"PI-121C","3#炉炉前集箱出口蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[17,"PI-103C","3#炉汽包就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[18,"PI-122C","3#炉省煤器出口水压就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[19,"PI-102-D","4#炉出口主蒸汽管就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[20,"PI-108-D","4#炉给水阀前就地压力表","0~6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[21,"PI-120-1D","4#炉炉前锅筒蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[22,"PI-120-2D","4#炉炉前集箱出口蒸汽就地压力表","0~4MPa","上海自动化仪表",{"$nulls":3},"A",1.6,6]
[23,"PI-103-D","4#炉汽包就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[24,"PI-129-2D","4#炉省煤器出口集箱就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[25,"PI-129-3D","4#炉省煤器出口水压就地压力表","0~4MPa","WIKA",{"$nulls":3},"A",1.6,6]
[26,"210-PI-053","吸附制氮机1#塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[27,"210-PI-054","吸附制氮机2#塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[28,"210-PI-GL1","4#空压机3#过滤器进口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[29,"210-PI-GL2","4#空压机3#过滤器出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[30,"210-PI-GL11","小空压机1#过滤器进口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[31,"210-PI-GL22","小空压机1#过滤器出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[32,"210-PI-1","3#空压机2#过滤器进口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[33,"210-PI-2","3#空压机2#过滤器出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[34,"210-PI-G3","3#冷干机油过滤器压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[35,"210-PI-052D","3#PS过滤器出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[36,"210-PI-052B","3#干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[37,"210-PI-052A","3#干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[38,"210-PI-052C","3#CS过滤器压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[39,"210-PI-MS3","4#冷干机MS3油过滤器压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[40,"210-PI-053D","4#PS过滤器出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[41,"210-PI-053B","4#干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[42,"210-PI-053A","4#干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[43,"210-PI-053C","4#CS过滤器压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[44,"210-PI-026","膜制氮装置空气储罐出口压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[45,"210-PI-048","吸附制氮机储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[46,"210-PI-046","吸附制氮机缓冲罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[47,"210-PI-1A","1#外加热再生干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[48,"210-PI-1B","1#外加热再生干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[49,"210-PI-2A","2#外加热再生干燥器A塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[50,"210-PI-2B","2#外加热再生干燥器B塔压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[51,"210-PI-121","2#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[52,"210-PI-120","1#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[53,"210-PI-123","4#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[54,"210-PI-122","3#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[55,"210-PI-124","6#缓冲罐压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[56,"210-PI-125","5#缓冲罐压缩空气压力（供界外）","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[57,"210-PI-063B","2#氮气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[58,"210-PI-062","卷曲机压缩空气压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[59,"210-PI-061A","1#空气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[60,"210-PI-061B","2#空气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[61,"210-PI-063A","1#氮气储罐压力","0~1.6MPa","WIKA",{"$nulls":3},"A",1.6,6]
[1,"压力表","1.6MPa","F18160320",{"$nulls":4},"B",1.6,12]
[2,"压力表","25MPa","F18160420",{"$nulls":4},"B",1.6,12]
[3,"压力表","1.6MPa","F04100721",{"$nulls":4},"B",0.4,12]
[4,"压力表","1.6MPa","F04100821",{"$nulls":4},"B",0.4,12]
[5,"压力表","4MPa","E26100021",{"$nulls":4},"B",0.4,12]
[6,"压力表","4MPa","E26100121",{"$nulls":4},"B",0.4,12]
[7,"压力表","16MPa","E20102321",{"$nulls":4},"B",0.4,12]
[8,"压力表","16MPa","E20102421",{"$nulls":4},"B",0.4,12]
[5,"PI-118","主蒸汽母管就地压力表","Y-150  0~4MPa"," ",{"$nulls":3},"A",1.6,12]
[4,"PT-369","4#给水泵出口压力变送器","0~4MPa",{"$nulls":4},"B",{"v":1,"d":"1.0"},"检修期 "]
[1,"氢气减压阀压力表","0-25MPa","上海减压器厂有限公司",{"$nulls":4},"B",4,6]
[2,"氧气减压阀压力表","0-25MPa","上海减压器厂有限公司",{"$nulls":4},"B",5,6]
[3,"氩气减压阀压力表","0-25MPa","上海减压器厂有限公司",{"$nulls":4},"B",2,6]
[4,"氮气减压阀压力表","0-25MPa","上海减压器厂有限公司",{"$nulls":4},"B",1,6]
[5,"乙炔减压阀压力表","0-25MPa","上海减压器厂有限公司",{"$nulls":4},"B",2,6]

{"sheet":"C类2025","index":1,"n_rows":1600,"n_cols":14,"rows_kept":1600}
["序号","仪表位号","设备名称","规格型号","制造厂商","分类","准确度","周期（月）",{"$nulls":3},"备注"]
[190,"PT-106-6A-2","1#炉送风机出口油压",null,null,"C"," "," "]
[188,"PT-107-6A-2","1#炉引风机出口油压",null,null,"C"," "," "]
[65,"PI-110B","2#炉减温阀后就地压力表","Y-150  0~6MPa",null,"C",null," "]
[66,"PI-111B","2#炉减温阀前就地压力表","Y-150  0~6MPa",null,"C",null," "]
[109,"PI-110C","3#炉减温阀后就地压力表","Y-150  0~6MPa",null,"C",null," "]
[110,"PI-111C","3#炉减温阀前就地压力表","Y-150  0~6MPa",null,"C",null," "]
[192,"PT-134D","4#炉送风机出口油压",null,null,"C"," "," "]
[194,"PT-132D","4#炉引风机出口油压",null,null,"C"," "," "]
[5,"TE-117-A","1#炉除尘器入口烟温(右)","#1锅炉(35t/h)",null,"C"]
[6,"TE-118-A","1#炉除尘器入口烟温(左)","#1锅炉(35t/h)",null,"C"]
[7,"LIA-101-A","1#炉电接点液位计","UDS-01S/15",null,"C"]
[8,"PI-109-A","1#炉给水阀后就地压力表","Y-150  0~6MPa",null,"C"]
[10,"TE-111-A","1#炉给水管双只铂热电阻","WZP2-630 PT100 225X75MM M33X2",null,"C"]
[11,"TI-102A","1#炉给水管温度双金属温度计","WSS-581B,0~150℃ L=75,d=10,M27X2","   ","C"]
[15,"TI-119-A","1#炉过热蒸汽出口集箱双金属温度计","WNG-11",null,"C"]
[16,"PI-111-A","1#炉减温阀后就地压力表","Y-150  0~6MPa",null,"C"]
[17,"FT-103-A","1#炉减温水流量计","R100S129NQBAMZZZZ/1700R12ABAMZZZPK","EMERSON","C"]
[19,"PI-121-A","1#炉空气预热器出口风压压力就地压力表右","Y-150  0~600Pa",null,"C"]
[26,"TE-112-A","1#炉炉膛入口风温(右)双只铂热电阻","WZP2-231 PT100 450X300mm M27X2","上海通控仪表有限公司","C"]
[37,"TI-108-A","1#炉省煤器出口水管温度双金属温度计","WSS-411，0~300℃，L=120","   ","C"]
[41,"TI-107-A","1#炉省煤器入口水水管双金属温度计","WSS-411，0~200℃，L=120，M27X2","   ","C"]
[44,"TE-113-A","1#炉送风机入口风温双只铂热电阻","WZP2-231 PT100 450X300mm M27X2","上海通控仪表有限公司","C"]
[46,"TI-102-A","1#炉主给水管双金属温度计","WSS-581B,0~150℃,L=75,d=10,M27X2","   ","C"]
[45,"FT-102-A","1#炉主给水流量计","R200SA37NQBAMZZZZ/1700R12ABAMZZZPK","EMERSON","C"]
[48,"FT-101-A","1#炉主蒸汽流量计","3095MFAS080CCHPS1T100T72CA1AG6M5F2","ROSEMOUNT","C"]
[51,"LIA-101B","2#炉电接点液位计","UDS-01S/15",null,"C"]
[53,"PI-109B","2#炉给水阀后就地压力表","Y-150  0~6MPa",null,"C"]
[55,"FT-102B","2#炉给水管流量变送器","R200SA37NQBAMZYZZ/1700R12ABAMZZZPK","EMERSON","C"]
[56,"TE-109B","2#炉给水管温度热电阻","WZP-630(K),Pt100",null,"C"]
[57,"TI-102B","2#炉给水管温度双金属温度计","WSS-581W,0~150℃","   ","C"]
[58,"TI-107B","2#炉给水混合器出口水管双金属温度计","WSS-581W,0~150℃","   ","C"]
[59,"PI-107-3B","2#炉给水就地压力表","Y-150  0~6MPa",null,"C"]
[70,"TE-111B","2#炉空气预热器后温度热电阻","WZP-330(K),Pt100",null,"C"]
[73,"TE-104B","2#炉炉膛出口温度热电偶","WRN-330(K),K",null,"C"]
[82,"TI-108B","2#炉省煤器出口水管温度双金属温度计","WSS-581W,0~200℃","   ","C"]
[85,"TE-106-1B","2#炉省煤器进口水管温度热电阻","WZP-630(K),Pt100",null,"C"]
[86,"TE-105B","2#炉省煤器前温度热电偶","WRN-330(K),E",null,"C"]
[88,"TE-113B","2#炉送风机出口风管温度热电阻","WZP-231(K),Pt100","上海通控仪表有限公司","C"]
[95,"LIA-101C","3#炉电接点液位计","UDS-01S/15",null,"C"]
[97,"PI-109C","3#炉给水阀后就地压力表","Y-150  0~4MPa",null,"C"]
[99,"FT-102C","3#炉给水管流量变送器","R200SA37NQBAMZYZZ/1700R12ABAMZZZPK","EMERSON","C"]
[100,"TE-109C","3#炉给水管温度热电阻","WZP-630(K),Pt100",null,"C"]
[101,"TI-102C","3#炉给水管温度双金属温度计","WSS-581W,0~150℃","   ","C"]
[102,"TI-107C","3#炉给水混合器出口水管双金属温度计","WSS-581W,0~150℃","   ","C"]
[103,"PI-107-3C","3#炉给水就地压力表","Y-150  0~6MPa",null,"C"]
[114,"TE-111C","3#炉空气预热器后温度热电阻","WZP-330(K),Pt100",null,"C"]
[117,"TE-104C","3#炉炉膛出口温度热电偶","WRN-330(K),K",null,"C"]
[126,"TI-108C","3#炉省煤器出口水管温度双金属温度计","WSS-581W,0~200℃","   ","C"]
[129,"TE-106-1C","3#炉省煤器进口水管温度热电阻","WZP-630(K),Pt100",null,"C"]
[130,"TE-105C","3#炉省煤器前温度热电偶","WRN-330(K),E",null,"C"]
[132,"TE-113C","3#炉送风机出口风管温度热电阻","WZP-231(K),Pt100","上海通控仪表有限公司","C"]
[142,"LIA-101-D","4#炉电接点液位计","UDS-01S/16",null,"C"]
[143,"PI-109-D","4#炉给水阀后就地压力表","Y-150  0~4MPa",null,"C"]
[145,"TI-102-D","4#炉给水管温度双金属温度计","WSS-581W,0~150","   ","C"]
[147,"TE-111-D","4#炉给水温度双只铂热电阻","WZP2-630 PT100 225X75MM M33X2",null,"C"]
[150,"TI-119-D","4#炉过热蒸汽出口集箱双金属温度计","WNG-11",null,"C"]
[151,"FT-103-D","4#炉减温水流量计","R100S129NQBAMZZZZ/1700R12ABAMZZZPK","EMERSON","C"]
[152,"PI-121-D","4#炉空气预热器出口风压压力就地压力表右","Y-150  0~600Pa",null,"C"]
[153,"PI-122-D","4#炉空气预热器出口风压压力就地压力表左","Y-150  0~600Pa",null,"C"]
[155,"TE-117-D","4#炉空预器入口风温（右）双只铂热电阻","WZP2-231 PT100 450X300mm M27X2","上海通控仪表有限公司","C"]
[156,"TE-118-D","4#炉空预器入口风温（左）双只铂热电阻","WZP2-231 PT100 450X300mm M27X2","上海通控仪表有限公司","C"]
[161,"TE-112-D","4#炉炉膛入口风温(右)",null,null,"C"]
[172,"TI-108-D","4#炉省煤器出口水管温度双金属温度计","WSS-411，0~300℃，L=120","   ","C"]
[176,"TI-107-D","4#炉省煤器入口水水管双金属温度计","WSS-411，0~200℃，L=120，M27X2","   ","C"]
[178,"TE-113-D","4#炉送风机出口风温",null,null,"C"]
[146,"FT-102-D","4#炉主给水流量计","R200SA37NQBAMZZZZ/1700R12ABAMZZZPK","EMERSON","C"]
[181,"FT-101-D","4#炉主蒸汽流量计","3095MFAS080CCHPS1T100T72CA1AG6M5F2","ROSEMOUNT","C"]
[184,"TI-504","一次母管蒸汽温度","0~500℃",null,"C"]
[185,"PI-504","一次母管蒸汽压力","0~4MPa",null,"C"]
[189,"PT-106-6A-1","1#炉送风机进口油压",null,null,"C",1]
[187,"PT-107-6A-1","1#炉引风机进口油压",null,null,"C",1]
[191,"PT-133D","4#炉送风机进口油压",null,null,"C",1]
[193,"PT-131D","4#炉引风机进口油压",null,null,"C",1]
[84,"PT-106B","2#炉省煤器后烟气负压压力变送器","1151GP3E,-800Pa~0Pa","ROSEMOUNT","C",1]
[87,"PT-105B","2#炉省煤器前烟气负压压力变送器","1151GP3E,-600Pa~0Pa","ROSEMOUNT","C",1,{"$nulls":4}," "]
[52,"FT-104B","2#炉风量流量变送器","1151DP,0~1kPa","ROSEMOUNT","C",1]
[68,"PT-113B","2#炉空气预热器出口风压压力变送器","1151GP4E,0~7kPa","ROSEMOUNT","C",1]
[89,"PT-112B","2#炉送风机出口风压压力变送器","1151GP4E,0~8kPa","ROSEMOUNT","C",1,{"$nulls":5},"4月提醒"]
[49,"PT-115B","2#炉除尘器后烟气负压压力变送器","1151GP3E,-3500Pa~0Pa","ROSEMOUNT","C",1]
[50,"PT-114B","2#炉除尘器前烟气负压压力变送器","1151GP3E,-3000Pa~0Pa","ROSEMOUNT","C",1]
[1,"PT-128-A","1#炉1#炉除尘器入口烟气压力 (左)","-7000Pa~0Pa","FOXBORO","C",1]
[3,"PT-115-A","1#炉除尘器后烟气负压压力变送器","-8000Pa~0Pa",null,"C",1]
[4,"PT-127-A","1#炉除尘器入口烟气压力(右)","-7000Pa~0Pa",null,"C",1]
[40,"PT-105-A","1#炉省煤器前烟气负压压力变送器","-8000Pa~0Pa","FOXBORO","C",1]
[42,"FT-104-A","1#炉送风风量差压变送器","0~1kPa","ROSEMOUNT","C",1]
[43,"PT-112-A","1#炉送风机出口风压压力变送器","0~6000Pa","FOXBORO","C",1]
[18,"PT-113-A","1#炉空气预热器出口风压压力变送器","0~5000Pa","FOXBORO","C",1]
[24,"PT-104-A","1#炉炉膛负压 1变送器","-200Pa~200Pa",null,"C",1]
[25,"PT-110-A","1#炉炉膛负压 2变送器","-200Pa~200Pa",null,"C",1]
[27,"PT-116-A","1#炉炉膛入口风压 (左)变送器","0~5000Pa","FOXBORO","C",1]
[131,"PT-105C","3#炉省煤器前烟气负压压力变送器","1151GP3E,-600Pa~0Pa","ROSEMOUNT","C",1,{"$nulls":4}," "]
[94,"PT-114C","3#炉除尘器前烟气负压压力变送器","1151GP3E,-3000Pa~0Pa","ROSEMOUNT","C",1]
[16,"PT-502","一次蒸汽压力变送器","1151GP8E,0~2.6MPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},36]
[17,"PT-503","一次蒸汽压力变送器","1151GP8E,0~2.6MPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},36]
[18,"PT-510","低压蒸汽出口压力变送器","3051CG5A22A1AM5B4DFK5 0~1.6MPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}," 检修期"]
[24,"PT-516","二次蒸汽压力变送器","1151GP6E,0~0.49MPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}," 检修期"]
[1,"FT-501","二次蒸汽1#热用户流量变送器","3095MFAS200ZCHPS2T100T71CA1AG2Q4M5F6","ROSEMOUNT","C"," "," "]
[5,"PI-506","二次蒸汽就地压力表","Y-150  0~2.5MPa",null,"C"," "," "]
[6,"PI-508","一次蒸汽压力变送器","Y-150  0~1MPa",null,"C"," "," "]
[7,"PI-509","二次蒸汽压力表","Y-150  0~1MPa",null,"C"," "," "]
[8,"PI-510","1#减温器出口就地压力表","Y-100  0~1MPa",null,"C"," "," "]
[9,"PI-511","2#减温器出口就地压力表","Y-100  0~1MPa",null,"C"," "," "]
[10,"PI-512","3#减温器出口就地压力表","Y-100  0~1MPa",null,"C"," "," "]
[15,"PT-501","一次蒸汽压力变送器","1151GP6E,0~0.49MPa","ROSEMOUNT","C"," "," "]
[26,"TE-304","2#除氧器水箱温度热电阻","WZP-231(K),Pt100",null,"C"," "," "]
[27,"TE-501","一次蒸汽温度","  ",null,"C"," "," "]
[28,"TE-501","一次蒸汽温度热电阻（双支）","WZP-230K",null,"C"," "," "]
[29,"TE-502","二次蒸汽温度","  ",null,"C"," "," "]
[30,"TE-502","二次蒸汽温度热电阻（双支）","WZP-230K",null,"C"," "," "]
[31,"TE-505","一次蒸汽温度热电阻（双支）","WZP-630K",null,"C"," "," "]
[32,"TE-506","二次蒸汽温度热电阻（双支）","WZP-630K",null,"C"," "," "]
[33,"TE-509","1#减温器出口温度","  ",null,"C"," "," "]
[34,"TE-509","1#减温器出口温度热电阻","WZP-230K",null,"C"," "," "]
[35,"TE-510","2#减温器出口温度","  ",null,"C"," "," "]
[36,"TE-510","2#减温器出口温度热电阻","WZP-230K",null,"C"," "," "]
[37,"TE-511","3#减温器出口温度","  ",null,"C"," "," "]
[38,"TE-511","3#减温器出口温度热电阻","WZP-230K",null,"C"," "," "]
[39,"TE-512","1#减温减压器出口温度","  ",null,"C"," "," "]
[40,"TE-512","1#减温减压器二次温度热电阻","WZP-630K",null,"C"," "," "]
[41,"TE-513","2#减温减压器出口温度","  ",null,"C"," "," "]
[42,"TE-513","2#减温减压器二次温度热电阻","WZP-630K",null,"C"," "," "]
[43,"TE-514","3#减温减压器出口温度","  ",null,"C"," "," "]
[44,"TE-514","3#减温减压器二次温度热电阻","WZP-630K",null,"C"," "," "]
[45,"TE-515","4#减温减压器出口温度","  ",null,"C"," "," "]
[46,"TE-515","4#减温减压器二次温度热电阻","WZP-630K",null,"C"," "," "]
[47,"TE-551","5#减温减压器出口双只热电阻","WZP2-231 PT100 225X75MM  M27X2",null,"C"," "," "]
[48,"TE-561","4#减温减压器出口双只热电阻","WZP2-231 PT100 250X100MM  M27X2",null,"C"," "," "]
[49,"TI-503","一次蒸汽温度双金属温度计","WSS-581W",null,"C"," "," "]
[50,"TI-504","一次蒸汽温度双金属温度计","WSS-581W  0~500℃",null,"C"," "," "]
[51,"TI-507","二次蒸汽温度双金属温度计","WSS-581W",null,"C"," "," "]
[52,"TI-508","二次蒸汽温度双金属温度计","WSS-581W  0~300℃",null,"C"," "," "]
[53,"TI-520","1#减温器出口金属套管温度计","WNG-12",null,"C"," "," "]
[54,"TI-521","2#减温器出口金属套管温度计","WNG-12",null,"C"," "," "]
[55,"TI-522","3#减温器出口金属套管温度计","WNG-12",null,"C"," "," "]
[15,"ANAT-1","阳床钠离子分析仪",9073,"HACH","C",null,1,{"$nulls":3},"见校验记录","维修日常比对无校验记录"]
[42,"FT-417","盐喷射器出口流量","1151DP4J 0-10kPa",null,"C",{"v":1,"d":"1.0"},36]
[1,"314-LIA-01","消防水池液位数显表","0-140INH2O",null,"C",1.6,12]
[10,"314-PIA-08","消防水总管压力数显表","0-1MPa",null,"C",1.6,12]
[11,"314-PIA-11","自来水总管压力数显表","Y-50 0-1MPa",null,"C",1.6,12]
[52,"LIA-407","废水回收池液位","0-4M",null,"C",1.6,12]
[77,"PDT-420","1#碳床过滤器进出口压差","1151DP",null,"C",{"v":1,"d":"1.0"},36]
[78,"PDT-421","2#碳床过滤器进出口压差","1151DP",null,"C",{"v":1,"d":"1.0"},36]
[79,"PDT-422","3#碳床过滤器进出口压差","1151DP",null,"C",{"v":1,"d":"1.0"},36]
[35,"FT-410","1#碳床过滤器进口流量","1151DP5J,0-10kPa",null,"C",{"v":1,"d":"1.0"},36]
[37,"FT-412","3#碳床过滤器进口流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[38,"FT-413","1#钠床过滤器进口流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[39,"FT-414","2#钠床过滤器进口流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[40,"FT-415","3#钠床过滤器进口流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[27,"FT-401","1#阳床入口流量","1151DP4J,0~25kPa",null,"C",{"v":1,"d":"1.0"},36]
[28,"FT-402","2#阳床入口流量","1151DP4J,0~25kPa",null,"C",{"v":1,"d":"1.0"},36]
[29,"FT-403","1#阴床入口流量","1151DP4J,0~25kPa",null,"C",{"v":1,"d":"1.0"},36]
[30,"FT-404","2#阴床入口流量","1151DP4J,0~25kPa",null,"C",{"v":1,"d":"1.0"},36]
[41,"FT-416","软化水泵出口母管流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[50,"FT-425","废液泵出口母管流量","1151DP ",null,"C",{"v":1,"d":"1.0"},36]
[36,"FT-411","2#碳床过滤器进口流量","1151DP5J,0~40kPa",null,"C",{"v":1,"d":"1.0"},36]
[13,"314-PT-01","消防水总管压力变送器  ","821GM-1S1SM2-AM,0.2~1MPa",null,"C",{"v":1,"d":"1.0"},36]
[2,"314-PI-03","1#消防泵出口就地压力表","Y-100  0-1MPa",null,"C",1.6,12]
[3,"314-PI-04","2#消防泵出口就地压力表","Y-100  0-1MPa",null,"C",1.6,12]
[4,"314-PI-05","柴油机泵出口就地压力表","Y-100  0-1MPa",null,"C",1.6,12]
[5,"314-PI-06","1#稳压泵出口就地压力表","Y-100  0-1MPa",null,"C",1.6,12]
[6,"314-PI-07","2#稳压泵出口就地压力表","Y-100  0-1MPa",null,"C",1.6,12]
[7,"314-PI-08","应急泵出口就地压力表","Y-150  0-1MPa",null,"C",1.6,12]
[8,"314-PI-09","应急泵母管就地压力表","Y-150  0-0.6MPa",null,"C",1.6,12]
[9,"314-PIA-01","自来水进水总就地压力表","Y-50 0-1MPa",null,"C",1.6,12]
[12,"314-PIS-02","消防水总管磁助电接点压力表","YYCA-150Z",null,"C",1.6,12]
[43,"FT-418","碳床至除盐水系统流量","1151DP4S  0-40kPa",null,"C",{"v":1,"d":"1.0"},36]
[137,"YDJ","软化水罐入口总管硬度仪","APA6000","HACH","C",null,1,{"$nulls":3},"见校验记录","停用设备"]
[18,"AT-401","阳床再生酸浓度计","1055-01-10-21","ROSEMOUNT","C"]
[19,"AT-403","阴床再生碱浓度计","1055-01-10-21","ROSEMOUNT","C"]
[20,"DCFT-1","酸流量电磁流量计",null,null,"C"]
[21,"DCFT-2 ","碱流量电磁流量计","  ",null,"C"]
[25,"DIA-405","钠床再生盐浓度计","1055-01-10-21",null,"C"]
[26,"ATO2","锅炉水在线溶氧仪","HK-318","北京华科仪","C"]
[31,"FT-405","1#除盐水泵出口流量"," ",null,"C"]
[44,"FT-419","钠床总出水旋涡流量计","4~20mA DC 24V",null,"C"]
[45,"FT-420","钠床总进水旋涡流量计","4~20mA DC 24V",null,"C"]
[46,"FT-421","1#除盐水系统出口旋涡流量计","4~20mA DC 24V",null,"C"]
[47,"FT-422","2#除盐水出口旋涡流量计","4~20mA DC 24V",null,"C"]
[48,"FT-423","活性碳过滤器出口旋涡流量计","4~20mA DC 24V",null,"C"]
[49,"FT-424","食堂蒸汽流量旋涡流量计","4~20mA DC 24V",null,"C"]
[51,"FT-452","化水清水进水电磁流量计","IMT25-PEAT302",null,"C"]
[53,"LI-JJLX","碱计量箱翻板液位计","0~100mm",null,"C"]
[54,"LI-sSJLX","酸计量箱翻板液位计","0~160mm",null,"C"]
[55,"LI-XFSC-1","1#消防水池液位","0~150mm",null,"C"]
[56,"LI-XFSC-2","2#消防水池液位","0~150mm",null,"C"]
[57,"LI-YJLX","盐计量箱玻璃管液位计","0~100mm",null,"C"]
[58,"LI-ZJSX-1","1#中间水箱玻璃管液位计","0~150mm",null,"C"]
[59,"LI-ZJSX-1FQ","1#中间水箱浮球液位开关","GSK-10-8",null,"C"]
[60,"LI-ZJSX-2","2#中间水箱玻璃管液位计","0-150mm",null,"C"]
[61,"LI-ZJSX-2FQ","2#中间水箱浮球液位开关","GSK-10-8",null,"C"]
[62,"LT-401","1#除盐水箱液位变送器","MPM416",null,"C"]
[63,"LT-402","2#除盐水箱液位变送器","UQK-75-50IIIG",null,"C"]
[64,"LT-403","清水箱液位变送器","UQK-75-50IIIG",null,"C"]
[65,"LT-404","1#软化水箱超声波液位计","0~5M",null,"C"]
[66,"LT-405","2#软化水箱超声波液位计","0~5M",null,"C"]
[67,"LT-420","化水中和池液位超声波液位计"," ",null,"C"]
[68,"LT-XFSC","消防水池液位","0~140inH2O",null,"C"]
[69,"LX-403","1#酸储罐浮球液位计"," ",null,"C"]
[70,"LX-403A","3#酸储罐超声波液位计","0~2m",null,"C"]
[71,"LX-404","2#酸储罐浮球液位计"," ",null,"C"]
[72,"LX-405","1#碱储罐超声波液位计","0~2m",null,"C"]
[73,"LX-406","2#碱储罐超声波液位计","0~2m",null,"C"]
[74,"LX-406A","3#碱储罐超声波液位计","0~2m",null,"C"]
[75,"LX-411","酸液计量箱超声波液位计","0~2m",null,"C"]
[76,"LX-413","碱液计量箱超声波液位计","0~1m",null,"C"]
[80,"PH-1","2#废液池ph计","1055-01-10-22","ROSEMOUNT","C"]
[82,"PH-3","1#废液池ph计","1055-01-10-22","ROSEMOUNT","C"]
[84,"PI-1#FYG","1#反应罐压力","Y-50 0~40PSI",null,"C"]
[85,"PI-2#FYG","2#反应罐压力","Y-50 0~40PSI",null,"C"]
[86,"PI-3#FYG","3#反应罐压力","Y-50 0~40PSI",null,"C"]
[87,"PI-4#FYG","4#反应罐压力","Y-50 0~40PSI",null,"C"]
[88,"PI-401","1#中间水泵出口就地压力表","Y-150  0~1MPa",null,"C"]
[89,"PI-402","2#中间水泵出口就地压力表","Y-150  0~1MPa",null,"C"]
[90,"PI-403","除盐系统再生泵出口就地压力表","Y-150  0~1MPa",null,"C"]
[91,"PI-404","1#除盐水泵出口就地压力表","Y-150  0~1MPa",null,"C"]
[92,"PI-405","2#除盐水泵出口就地压力表","Y-150  0~1MPa",null,"C"]
[93,"PI-406","1#废液泵出口就地膜片式压力表","Y-150  0~1MPa",null,"C"]
[94,"PI-407","2#废液泵出口就地膜片式压力表","Y-150  0~1MPa",null,"C"]
[95,"PI-408","除盐水母管就地压力表","Y-150  0~1MPa",null,"C"]
[96,"PI-411","碱泵出口就地膜片式压力表","Y-150  0~1MPa",null,"C"]
[97,"PI-412","软化系统进口总管就地压力表","YXC-150  0~1MPa",null,"C"]
[98,"PI-413","软化系统反洗泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[99,"PI-414","1#清水泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[100,"PI-415","2#清水泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[101,"PI-416","3#清水泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[102,"PI-417","至除盐系统软化水就地压力表","YXC-150  0~1MPa",null,"C"]
[103,"PI-418","盐液出口就地膜片式压力表","Y-150  0~1MPa",null,"C"]
[104,"PI-419","1#软化水泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[105,"PI-420","2#软化水泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[106,"PI-421","软化系统再生泵出口就地压力表","YXC-150  0~1MPa",null,"C"]
[107,"PI-422","软化水总管就地压力表","YXC-150  0~1MPa",null,"C"]
[108,"PI-423","1#阳离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[109,"PI-424","1#阳离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[110,"PI-425","2#阳离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[111,"PI-426","2#阳离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[112,"PI-427","1#阴离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[113,"PI-428","1#阴离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[114,"PI-429","2#阴离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[115,"PI-430","2#阴离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[116,"PI-431","1#活性碳过滤器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[117,"PI-432","1#活性碳过滤器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[118,"PI-433","2#活性碳过滤器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[119,"PI-434","2#活性碳过滤器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[120,"PI-435","3#活性碳过滤器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[121,"PI-436","3#活性碳过滤器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[122,"PI-437","1#钠离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[123,"PI-438","1#钠离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[124,"PI-439","2#钠离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[125,"PI-440","2#钠离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[126,"PI-441","3#钠离子交换器入口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[127,"PI-442","3#钠离子交换器出口就地膜片式压力表","Y-100  0~1MPa",null,"C"]
[128,"PI-443","清水箱出口就地压力表","Y-100  0~1MPa",null,"C"]
[130,"PI-jrsg","加热水罐压力","Y-100  0~1MPa",null,"C"]
[131,"PI-xfsc","消防水池进水压力","Y-50 0~40PSI",null,"C"]
[135,"STYL-1","食堂","Y-150  0~0.4MPa",null,"C"]
[136,"STYL-2","食堂","Y-100  0~1.6MPa",null,"C"]
[22,"DT-403","1#阴床出水电导","8225-FPM-PVDF-55",null,"C"]
[23,"DT-404","2#阴床出水电导","8225-FPM-PVDF-55",null,"C"]
[24,"DT-405","除盐水总管电导","8225-FPM-PVDF-55",null,"C"]
[2,"PI-1-1","1#脱水仓压力表1","0~0.6MPa"," ","C"]
[3,"PI-1-2","1#脱水仓压力表2","0~0.6MPa"," ","C"]
[4,"PI-2-1","2#脱水仓压力表1","0~0.6MPa"," ","C"]
[5,"PI-2-2","2#脱水仓压力表2","0~0.6MPa"," ","C"]
[6,"DDC-TE-01","1#前电场灰斗热电偶","E型"," ","C"]
[7,"DDC-TE-02","1#中电场灰斗热电偶","E型"," ","C"]
[8,"DDC-TE-03","1#中大梁2加热热电偶","E型"," ","C"]
[9,"DDC-TE-04","1#后大梁加热热电偶","E型"," ","C"]
[10,"DDC-TE-05","1#前大梁加热热电偶","E型"," ","C"]
[11,"DDC-TE-06","1#中大梁1加热热电偶","E型"," ","C"]
[12,"DDC-TE-07","2#前电场灰斗热电偶","E型"," ","C"]
[13,"DDC-TE-08","2#中电场灰斗热电偶","E型"," ","C"]
[14,"DDC-TE-09","2#阴极瓷轴加热热电偶","E型"," ","C"]
[15,"DDC-TE-10","2#进出口封斗热电偶","E型"," ","C"]
[16,"DDC-TE-11","2#中大梁2加热热电偶","E型"," ","C"]
[17,"DDC-TE-12","2#后大梁加热热电偶","E型"," ","C"]
[18,"DDC-TE-13","2#前大梁加热热电偶","E型"," ","C"]
[19,"DDC-TE-14","2#中大梁1加热热电偶","E型"," ","C"]
[20,"DDC-TE-15","3#后电场灰斗热电偶","E型"," ","C"]
[21,"DDC-TE-16","3#前电场灰斗热电偶","E型"," ","C"]
[22,"DDC-TE-17","3#中电场灰斗热电偶","E型"," ","C"]
[23,"DDC-TE-18","3#阴极瓷轴加热热电偶","E型"," ","C"]
[24,"DDC-TE-19","3#进出口封斗热电偶","E型"," ","C"]
[25,"DDC-TE-20","3#中大梁2加热热电偶","E型"," ","C"]
[26,"DDC-TE-21","3#后大梁加热热电偶","E型"," ","C"]
[27,"DDC-TE-22","3#前大梁加热热电偶","E型"," ","C"]
[28,"DDC-TE-23","3#中大梁1加热热电偶","E型"," ","C"]
[29,"DDC-TE-24","4#前电场灰斗热电偶","E型"," ","C"]
[30,"DDC-TE-25","4#中电场灰斗热电偶","E型"," ","C"]
[31,"DDC-TE-26","4#中大梁2加热热电偶","E型"," ","C"]
[32,"DDC-TE-27","4#后大梁加热热电偶","E型"," ","C"]
[33,"DDC-TE-28","4#前大梁加热热电偶","E型"," ","C"]
[34,"DDC-TE-29","4#中大梁1加热热电偶","E型"," ","C"]
[35,"LT-01","1#脱水仓物位计","VEGAPULS  52K"," ","C"]
[36,"LT-02","2#脱水仓物位计","VEGAPULS  52K"," ","C"]
[37,"LT-03","1#煤仓物位计","VEGAPFLEX  65"," ","C"]
[38,"LT-04","2#煤仓物位计","VEGAPFLEX  65"," ","C"]
[39,"LT-05","3#煤仓物位计","VEGAPFLEX  65"," ","C"]
[40,"LT-06","4#煤仓物位计","VEGAPFLEX  65"," ","C"]
[41,"TIA-721","2#前电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X72-HL)","余姚仪表厂","C"]
[42,"TIA-722","2#中电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X73-HL)","余姚仪表厂","C"]
[43,"TIA-723","2#后电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X74-HL)","余姚仪表厂","C"]
[44,"TIA-724","2#前大梁加热温度显示仪","ＸＭＴ数显调节仪（横-144X75-HL)","余姚仪表厂","C"]
[45,"TIA-725","2#中大梁1加热温度显示仪","ＸＭＴ数显调节仪（横-144X76-HL)","余姚仪表厂","C"]
[46,"TIA-726","2#中大梁2加热温度显示仪","ＸＭＴ数显调节仪（横-144X77-HL)","余姚仪表厂","C"]
[47,"TIA-727","2#后大梁加热温度显示仪","ＸＭＴ数显调节仪（横-144X78-HL)","余姚仪表厂","C"]
[48,"TIA-728","2#巡检仪温度显示仪","ＸＭＴ数显调节仪（横-144X79-HL)","余姚仪表厂","C"]
[49,"TIA-731","3#前电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X80-HL)","余姚仪表厂","C"]
[50,"TIA-732","3#中电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X81-HL)","余姚仪表厂","C"]
[51,"TIA-733","3#后电场灰斗温度显示仪","ＸＭＴ数显调节仪（横-144X82-HL)","余姚仪表厂","C"]
[52,"TIA-734","3#前大梁加热温度显示仪","ＸＭＴ数显调节仪（横-144X83-HL)","余姚仪表厂","C"]
[53,"TIA-735","3#中大梁1加热温度显示仪","ＸＭＴ数显调节仪（横-144X84-HL)","余姚仪表厂","C"]
[54,"TIA-736","3#中大梁2加热温度显示仪","ＸＭＴ数显调节仪（横-144X85-HL)","余姚仪表厂","C"]
[55,"TIA-737","3#后大梁加热温度显示仪","ＸＭＴ数显调节仪（横-144X86-HL)","余姚仪表厂","C"]
[56,"TIA-738","3#巡检仪温度显示仪","ＸＭＴ数显调节仪（横-144X87-HL)","余姚仪表厂","C"]
[58,"FT-PDC-01","皮带秤","SV-805S","赛摩力拓","C",null,"周期按工艺需求",{"$nulls":3},"周期按工艺需求","按实际需求校验"]
[63,"210-PI-045","吸附制氮压缩空气进气压力","0~1.6MPa","WIKA","C",1.6]
[90,"210-PI-216","3#空压机出气压力","0~1.0MPa","WIKA","C",1.6]
[101,"210-PI-209A","4#空压机出气压力","0~1.0MPa","WIKA","C",1.6]
[115,"210-PI-224","3#冷干机出气压力","0~1.0MPa","WIKA","C",1.6]
[117,"210-PI-223","3#冷干机进气压力","0~1.6MPa","WIKA","C",1.6]
[128,"210-PI-220","4#冷干机出气压力","0~1.0MPa","WIKA","C",1.6,{"$nulls":4}," "]
[198,"350-PT-01","砂过滤器压力","DP6E22M3B3C2,  0~250kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[53,"210-PT-201","冷却水回水总管压力","IGP20-T22D21F-M1L1 0~0.5MPa","FOXBORO公司","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[172,"312-PT-01","工艺冷却水出水总管压力","STG944-AIG-00000.CC.M13","HONEYWELL ST3000","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[141,"210-PT-109","压缩空气总管压力","1151GP7S12M1B3D2  0~300PSI","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[226,"COD-1","在线COD分析仪","WQ1000","深圳正奇环境科技有限公司","C",{"$nulls":5},"见校验记录"]
[1,"210-PI-115","1#冷水机冷却回水压力","0~0.6MPa","上海自动化仪表四厂","C"]
[2,"210-PI-114","1#冷水机冷却供水压力","0~0.6MPa","杭州、雷尔达仪表公司","C"]
[3,"210-TI-111","冷却水回水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[4,"210-TI-112","冷却水供水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[5,"210-PI-056","1#冷水机出水压力","0~0.6MPa","青岛四方仪表厂","C"]
[6,"210-TI-114","1#冷水机出水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[7,"210-PI-055","冷冻水进口压力","0~1.5MPa","WIKA","C"]
[8,"210-TI-103","冷冻水进口温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[9,"210-PT-113","冷冻水供水压力","3051S1TG2A2E11A1AB4D1M5,0~100kPa","ROSEMONT公司","C"," "," "]
[10,"210-PI-110","1#冷水泵出口压力","0~1.0MPa","WIKA","C"]
[11,"210-PI-111","2#冷水泵出口压力","0~1.0MPa","WIKA","C"]
[12,"210-PI-112","3#冷水泵出口压力","0~1.6MPa","青岛四方仪表厂","C"]
[13,"210-LT-101","冷冻水池液位","DB101 G1TE202M,0~2.5M","北京E+H公司","C"]
[14,"210-TE-109","冷冻水出水总管温度","PT100",null,"C"]
[15,"210-PI-116","2#冷水机冷却水供水压力","0~0.6MPa","杭州、雷尔达仪表公司","C"]
[16,"210-TI-110","2#冷水机冷却水供水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[17,"210-TI-113","冷却水回水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[18,"210-PI-117","冷却水回水压力","0~0.6MPa","上海仪表四厂","C"]
[19,"210-PI-057","2#机出水压力","0~1.0MPa","青岛四方仪表厂","C"]
[20,"210-TI-115","2#机出水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[21,"210-FT-102","一期冷冻水流量","F9286AJ  0~300NM3/H","YOKOGAWA SHANGHAI","C"]
[22,"210-PI-104","冷却水回水压力","0~1.0MPa","WIKA","C"]
[23,"210-PI-103","冷却水回水压力","0~1.0MPa","WIKA","C"]
[24,"210-TI-104","冷却水回水温度","WSS-481W  0~100℃","上海仪表四厂","C"]
[25,"FT-204","一期冷冻水池补充水流量","F-T02S1SSTNA          ","FOXBORO公司","C"]
[26,"210-PI-209","4#冷冻水泵出口压力","0~1.0MPa","西安仪表厂","C"]
[27,"210-PI-210","5#冷冻水泵出口压力","0~1.0MPa","上海仪表四厂","C"]
[28,"210-PI-211","6#冷冻水泵出口压力","0~1.0MPa","西安仪表厂","C"]
[29,"210-PE-01","补水泵出口电接点压力表","YX150  0~1.0MPa            ","青岛华青集团有限公司","C"]
[30,"210-PT-204","冷却水出水压力","IGP20-T22D21F-M1L1","FOXBOR","C"]
[31,"210-PT-203","冷却水进水压力","IGP20-T22D21F-M1L1","FOXBOR","C"]
[32,"210-TE-203","冷却水进水温度","PT100",null,"C"]
[33,"210-TE-204","冷却水出水温度","PT100",null,"C"]
[34,"FT-202","二期冷却水进口电磁流量计","IMT25-PEATB10K   240VAC 30VA","FOXBORO公司","C"]
[35,"FT-109","二期丝束总管电磁流量计","IMT25-PEATB10Z   240VAC 30VA","FOXBORO公司","C"]
[36,"210-PI-205","3#冷水机冷却水进水压力","0~0.6MPa","上海自动化仪表四厂","C"]
[37,"210-TI-205","3#冷水机冷却水进水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[38,"210-TI-206","3#冷水机冷却水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[39,"210-PI-206","3#冷水机冷却水出水压力","0~0.6MPa","西安仪表厂","C"]
[40,"210-TI-208","3#冷水机冷冻水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[41,"210-PI-208","3#冷水机冷冻水出水压力","0~0.6MPa","上海自动化仪表四厂","C"]
[42,"210-PI-207","3#冷水机冷冻水回水压力","0~1.0MPa","西安仪表厂","C"]
[43,"210-TI-207","3#冷水机冷冻水回水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[44,"210-PI-201","4#冷水机冷却水进水压力","0~0.6MPa","上海自动化仪表四厂","C"]
[45,"210-TI-201","4#冷水机冷却水进水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[46,"210-TI-202","4#冷水机冷却水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[47,"210-PI-202","4#冷水机冷却水出水压力","0~1.0MPa","西安仪表厂","C"]
[48,"210-TI-203","4#冷水机冷冻水进水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[49,"210-TI-204","4#冷水机冷冻水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[50,"210-PI-203","4#冷水机冷冻水回水压力","0~1.0MPa","上海自动化仪表四厂","C"]
[51,"210-PI-204","4#冷水机冷冻水出水压力","0~1.0MPa","西安仪表厂","C"]
[54,"FT-201","二期冷冻水总管电磁流量计","IMT25-PEATB10K   240VAC 30VA","FOXBORO公司","C"]
[55,"TE-202","二期冷冻水总管温度","PT100",null,"C"]
[56,"TE-204","二期冷冻水回水总管温度","PT100",null,"C"]
[57,"TE-201","低温回水总管温度","PT100",null,"C"]
[59,"210-PI-042","膜机组出口压力","0~1400kPa","WIKA","C"]
[60,"210-PI-041","膜机组进口压力","0~160PSI","WIKA","C"]
[61,"210-ATI-002","氧分析仪","329R",null,"C"]
[62,"210-ATI-002-1","氧分析仪","Z0A--200  0~25%","中国南京长鼎","C"]
[64,"210-PI-047","仪表空气压力","0~160PSI","WIKA","C"]
[65,"210-PI-050","吸附制氮机储罐出口压力","0~160PSI","WIKA","C"]
[66,"210-PI-051","1#塔平衡压力","0~1kg/cm2   0~160PSI","ASHCROFT","C"]
[69,"210-PI-052","1#塔平衡压力","0~1kg/cm2   0~160PSI","ASHCROFT","C"]
[70,"210-PI-049","吸附制氮机吸附塔出口压力","0~1kg/cm2   0~160PSI","ASHCROFT","C"]
[73,"210-AT-001","氧分析仪","100-0-0-2100-00",null,"C"]
[74,"210-TE-011","1#机一级排气温度","PT100   WZPK-230","云南仪表厂","C"]
[75,"210-TE-012","1#机二级排气温度","PT100   WZPK-230","云南仪表厂","C"]
[76,"210-PI-027","1#机冷却水压力","0~1.0MPa","WIKA","C"]
[77,"210-TI-105","1#机回水温度","WSS-481W   0~100℃","上海虹达仪器仪表厂","C"]
[78,"210-TE-102","后冷却器出口温度","PT100",null,"C"]
[79,"210-TE-021","2#机一级排气温度","PT100   WZPK-230","云南仪表厂","C"]
[80,"210-TE-022","2#机二级排气温度","PT100   WZPK-230","云南仪表厂","C"]
[81,"210-PI-029","2#机冷却水压力","0~1.0MPa","WIKA","C"]
[82,"210-TI-108","2#机冷却水温度","WSS-481W  0~100℃","上海虹达仪器仪表厂","C"]
[83,"210-TE-104","后冷却器出口温度","PT100",null,"C"]
[86,"210-PI-218","二级进气压力","0~1MPa","西安仪表厂","C"]
[87,"210-TI-218","二级进气温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[88,"210-TI-213","二级出气温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[89,"210-PI-213","二级出气压力","0~1MPa","西安仪表厂","C"]
[91,"210-TI-212","一级进气温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[94,"210-TI-210","4#空压机冷却水进水温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[95,"210-PI-214","4#空压机冷却水进水压力","0~1.6MPa","西安仪表厂","C"]
[96,"210-TI-211","4#空压机冷却水出水温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[97,"210-PI-215","4#空压机冷却水出水压力","0~1.6MPa","西安仪表厂","C"]
[100,"210-TI-209","4#空压机出气温度","WSS-481W   0~60℃","上海自动化仪表三厂","C"]
[106,"210-TI-033","B塔进气温度","WSS-481W   0~300℃","广东肇庆温度仪表厂","C"]
[107,"210-TI-034","B塔出气温度","WSS-481W   0~300℃","广东肇庆温度仪表厂","C"]
[108,"210-TI-031","A塔进气温度","WSS-481W   0~300℃","广东肇庆温度仪表厂","C"]
[109,"210-TI-032","A塔出气温度","WSS-481W   0~300℃","广东肇庆温度仪表厂","C"]
[110,"210-TI-036","A塔出气温度","WSS-481W   0~300℃","上海虹达仪器仪表厂","C"]
[111,"210-TI-035","A塔进气温度","WSS-481W   0~300℃","上海虹达仪器仪表厂","C"]
[112,"210-TI-037","B塔进气温度","WSS-481W   0~300℃","上海虹达仪器仪表厂","C"]
[113,"210-TI-038","B塔出气温度","WSS-481W   0~300℃","上海虹达仪器仪表厂","C"]
[114,"210-TI-220","3#冷干机出气温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[118,"210-TI-219","3#冷干机进气温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[123,"210-TI-225","3#冷干机冷却水进水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[124,"210-TI-226","3#冷干机冷却水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[125,"210-PI-225","3#冷干机冷却水进水压力","0~0.6MPa","西安仪表厂","C"]
[126,"210-PI-226","3#冷干机冷却水出水压力","0~0.6MPa","西安仪表厂","C"]
[127,"210-TI-216","4#冷干机出气温度"," WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[130,"210-PI-219","4#冷干机进气压力","0~1.0MPa","上海仪表四厂","C"]
[131,"210-TI-215","4#冷干机进气温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[136,"210-TI-221","4#冷干机冷却水进水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[137,"210-TI-222","4#冷干机冷却水出水温度","WSS-481W   0~60℃","上海自动化仪表四厂","C"]
[138,"210-PI-221","4#冷干机冷却水进水压力","0~0.6MPa","西安仪表厂","C"]
[139,"210-PI-222","4#冷干机冷却水出水压力","0~0.6MPa","西安仪表厂","C"]
[148,"210-LT-200","液氮液位计","XMZ-203","四川空气分离设备厂","C"]
[149,"210-PI-300","液氮氧压力表","0~1.6MPa",null,"C"]
[151,"210-FT-101","压缩空气流量","83W-T06S1SSTJA","FOXBORO","C"]
[152,"FT-203","至卷曲机压缩空气流量","3051SFADG050CCHPS1T100031AA1A2RLM5","ROSEMOUNT","C"]
[154,"FT-205","至废水、脱硫、出渣压缩空气流量","83F-T03S1SSTNT","FOXBORO","C"]
[155,"FT-206","至热电站压缩空气流量","83F-T03S1SSTNT","FOXBORO","C"]
[156,"FT-207","至化水、烟气压缩空气流量","83F-T03S1SSTNT","FOXBORO","C"]
[157,"210-FT-103","氮气流量","F9286AJ   YF04120511  ","上海横河","C"]
[158,"PT-205","压缩空气总管压力","IGP20-T22D21F-M1L1","FOXBOR","C"]
[159,"313-PI-01","1#丝束循环水泵出口压力","0~1.0MPa","漳洲仪表厂","C"]
[160,"313-PI-02","2#丝束循环水泵出口压力","0~1.0MPa","漳洲仪表厂","C"]
[161,"313-PI-03","3#丝束循环水泵出口压力","0~1.0MPa","WIKA","C"]
[162,"313-PI-05","5#丝束循环水泵出口压力","0~1.6MPa","上海自动化仪表四厂","C"]
[163,"313-PI-06","6#丝束循环水泵出口压力","0~1.0MPa","漳洲仪表厂","C"]
[164,"313-PI-04","4#丝束循环水泵出口压力","0~1.6MPa","上海自动化仪表四厂","C"]
[165,"312-PI-05","9#丝束循环水泵出口压力","0~1.0MPa","漳洲仪表厂","C"]
[166,"312-PI-04","8#丝束循环水泵出口压力","0~1.0MPa","青岛四方仪表厂","C"]
[167,"312-PI-06","7#丝束循环水泵出口压力","0~1.0MPa","四川昆仑仪表厂","C"]
[168,"312-PI-03","6#丝束循环水泵出口压力","0~1.6MPa","西安仪表厂","C"]
[170,"FT-104","1#丝束水池补水流量","83W-T04S1SSTJA","FOXBORO公司","C"]
[171,"312-LT-01","312冷水塔液位","DB101-G1 TE202M   3M","北京E+H公司","C"]
[173,"313-LT-01","313冷水塔液位","DB101-G1 TE202M   3M","北京E+H公司","C"]
[174,"312-PI-12","1#冷却塔进水阀压力","0~0.25MPa","WIKA","C"]
[175,"312-PI-13","2#冷却塔进水阀压力","0~1.0MPa","WIKA","C"]
[176,"312-PI-14","3#冷却塔进水阀压力","0~0.25MPa","WIKA","C"]
[177,"312-PI-15","4#冷却塔进水阀压力","0~1.0MPa","上海自动化仪表四厂","C"]
[178,"312-PI-16","5#冷却塔进水阀压力","0~1.0MPa","WIKA","C"]
[179,"FT-103","冷却水排污流量","IMT25-PEATB10K","FOXBORO公司","C"]
[180,"313-PI-17","9#冷却塔进水阀压力","0~1.0MPa","WIKA","C"]
[181,"313-PI-18","10#冷却塔进水阀压力","0~1.0MPa","WIKA","C"]
[182,"FT-105","丝束3#水池软化水补水流量","83W-T04S1SSTJA","FOXBORO公司","C"]
[183,"512-TE-1","丝束冷却塔6#风机温度","PT100",null,"C"]
[184,"512-TE-2","丝束冷却塔7#风机温度","PT100",null,"C"]
[185,"512-TE-3","丝束冷却塔8#风机温度","PT100",null,"C"]
[186,"FT-106","动力站进口冷却水流量","IMT25-PEATB10K","FOXBORO公司","C"]
[187,"312-PI-10","加药池压力","0~0.25MPa","WIKA","C"]
[188,"312-LTI-01","加药池液位计","TZP型磁性浮子液位计   L=0.675M   ","宜兴市新洲环保有限公司","C"]
[189,"350-PI-307","1#风机出口压力","0~0.25MPa","WIKA","C"]
[190,"350-PI-308","2#风机出口压力","0~0.25MPa","WIKA","C"]
[191,"350-PI-304","1#废水泵出口压力","0~0.25MPa","WIKA","C"]
[192,"350-PI-305","2#废水泵出口压力","0~0.25MPa","WIKA","C"]
[193,"350-LT-310","1#废水池超声波液位计","LU20-5001","CE公司","C"]
[194,"350-LT-311","2#废水池超声波液位计","LU20-5001","CE公司","C"]
[195,"350-FT-301","废水出口流量","AE210MG","ADMAG   AE公司","C"]
[196,"350-LT-301","集水井液位计（三线制）","7ML1201-2EE00  0~3M","加拿大 NRTL/C公司","C"]
[197,"FWT-350","中水流量计","7ME5038-2AA12-A1AA0","SIEMENTS","C"]
[199,"350-PI-4","4#管道泵出口压力","0~1MPa","上海荣华仪表厂","C"]
[200,"350-PI-3","3#管道泵出口压力","0~1MPa","上海荣华仪表厂","C"]
[201,"350-PI-1","1#中间水泵出口压力","0~1MPa","上海荣华仪表厂","C"]
[202,"350-PI-2","2#中间水泵出口压力","0~1MPa","上海荣华仪表厂","C"]
[203,"PIW-340","废水浊度仪","1720E+sc200","HACH","C"]
[204,"350-WN-1","污泥界面仪",null,null,"C"]
[205,"350-PI-103","热电站循环水进水总管压力","0~1.6PSI","西安仪表厂","C"]
[206,"350-PT-104","热电站循环水进水总管压力","1GP20-T22021F-M1L1,0~700kPa","FOXBOR公司","C"]
[207,"TE-105","热电站循环水出水总管温度","PT100",null,"C"]
[208,"350-PI-105","热电站循环水出水总管压力","0~1.6PSI","西安仪表厂","C"]
[209,"350-PT-105","热电站循环水出水总管压力","0~1.6PSI","FOXBORO","C"]
[210,"TE-104","热电站循环水进水总管温度","PT100",null,"C"]
[211,"350-PT-103","热电站循环水出水总管压力","1GP20-T22021F-M1L1","FOXBOR","C"]
[212,"350-LT-103","热电站循环水水池液位","VEGAFLEX65 0~2.5M","VEGA","C"]
[213,"FT-107","热电站循环水总管流量","IMT25-PEATB10K","FOXBORO","C"]
[214,"313-PI-101","热电1#循环水泵出口压力","0~1MPa","上海自动化仪表四厂","C"]
[215,"313-PI-102","热电2#循环水泵出口压力","0~1MPa","上海自动化仪表四厂","C"]
[216,"313-PI-103","热电3#循环水泵出口压力","0~1MPa","上海自动化仪表四厂","C"]
[217,"313-PI-104","热电4#循环水泵出口压力","0~1MPa","上海自动化仪表四厂","C"]
[218,"313-PI-105","热电5#循环水泵出口压力","0~1MPa","上海自动化仪表四厂","C"]
[219,"FT-108","热电自来水补水流量","83F-T03S1SSTNA","FOXBOR公司","C"]
[220,"313-TE-1","1#热电风机温度","PT100","上海仪表厂","C"]
[221,"313-TE-2","2#热电风机温度","PT100","上海仪表厂","C"]
[222,"313-TE-3","3#热电风机温度","PT100","上海仪表厂","C"]
[223,"350-PI-046","1#污水提升泵出口压力","0~1.6MPa","青岛四方仪表厂","C"]
[224,"350-PI-047","2#污水提升泵出口压力","0~1.0MPa","上海荣华仪表厂","C"]
[363,"PT","08-0209","摆丝机顶杆供液管压力变送器","1151GP8S12I5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[133,"FT","07-0127","1#干燥机去1区喷雾蒸汽流量变送器","3051S1CD3A2A11A1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[155,"FT   ","07-0227","2#干燥机去1区喷雾蒸汽流量变送器","3051S1CD3A2A11A1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[1,"PT   ","11-0009","1# 纺丝机预热空气压力变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6.6降为C类"]
[416,"PT","08-2208","摆丝液压压力变送器","3051S1TG3A2E11A1AB4D","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[26,"LT   ","06-0212","SI-90乳剂槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[29,"LT   ","06-0220","SI-90供给槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[384,"PT   ","11-0001","2# 纺丝机预热空气压力变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4},"2025年6月4日维修赵继彬要求降为C类"]
[30,"LT   ","06-0221","ST-90无离子水储槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[31,"LT   ","06-0222","过氧化物供给槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[409,"PT","11-2001","4# 纺丝机预热空气压力变送器",null,"ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[410,"PT","11-2009","3# 纺丝机预热空气压力变送器",null,"ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[52,"FT   ","06-0321","纺丝机1A面竖管VLA流量变送器   ","3051CD1A22A1AB4M5E4","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[39,"FT   ","06-0242","换热器进口脱离子水流量变送器       ","1151DP4S12I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[55,"FT   ","06-0324","纺丝机2B面竖管VLA流量变送器   ","3051CD1A22A1AB4M5E4","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[402,"FT","18-0002","1#干燥机入口排气流量变送器","3051CD1A52A1A  0~0.2kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[53,"FT   ","06-0322","纺丝机1B面竖管VLA流量变送器  ","3051CD1A22A1AB4M5E4 0~1.946kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[54,"FT   ","06-0323","纺丝机2A面竖管VLA流量变送器  ","3051CD1A22A1AB4M5E4 0~0.585kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[403,"FT","18-0005","2#干燥机 入口排气流量变送器","3051CD1A52A1A   0~0.2kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[34,"PT ","06-0231","1~8#卷曲机去离子水压力变送器","3051S  0~490.322kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[35,"PT","06-0232","9~16#卷曲机去离子水压力变送器","3051S  0~490.322kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[82,"PT","06-2231","卷曲机压缩空气总管压力变送器"," ","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[84,"PT","06-2232","25~32#卷曲机去离子水压力变送器"," ","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[367,"PI","08-0338","压力表  ","0~600PSI","WIKA","C",2.5]
[368,"PI","08-0339","压力表  ","0~600PSI","WIKA","C",2.5]
[369,"PI","08-0342","压力表  ","0~600PSI","WIKA","C",2.5]
[370,"PI","08-A01","打包A系统#1泵油压","0~5000PSI","WIKA","C",2.5]
[371,"PI","08-A02","打包A系统#2泵油压","0~5000PSI","WIKA","C",2.5]
[372,"PI","08-A03","打包A系统#3泵油压","0~5000PSI","WIKA","C",2.5]
[373,"PI","08-A04","打包A系统#4泵油压","0~5000PSI","WIKA","C",2.5]
[374,"PI","08-A05","打包A系统#5泵油压","0~5000PSI","WIKA","C",2.5]
[375,"PI","08-A06","打包A系统#6泵油压","0~5000PSI","WIKA","C",2.5]
[376,"PI","08-A07","打包A系统过滤冷却器泵压","0~200PSI","WIKA","C",2.5]
[377,"PI","08-B01","打包B系统#1泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[378,"PI","08-B02","打包B系统#2泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[379,"PI","08-B03","打包B系统#3泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[380,"PI","08-B04","打包B系统#4泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[381,"PI","08-B05","打包B系统#5泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[382,"PI","08-B06","打包B系统#6泵油压","0~6000PSI/0-400bar","WIKA","C",2.5]
[383,"PI","08-B07","打包B系统过滤冷却器泵压","0~200PSI","WIKA","C",2.5]
[364,"AI","08-0302","丝束包水份数显仪","WP-N80","国产","C",{"v":1,"d":"1.0"}]
[2,"TI   ","06-0001","温度计","50EI60E060          ","ASHCROFT","C"," "]
[3,"PI-A ","06-0010","差压计  ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[4,"PI-B ","06-0010","差压计   ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[5,"PI-A ","06-0024","差压计","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[6,"PI-B ","06-0024","差压计 ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[7,"TI   ","06-0034","温度计  ","50EI60E060          ","ASHCROFT","C"," "]
[8,"PI-A ","06-0043","差压计  ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[9,"PI-B ","06-0043","差压计   ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[10,"PI-A ","06-0057","差压计","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[11,"PI-B ","06-0057","差压计 ","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[12,"PSH  ","06-0065","纺丝机2B面VLA压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[13,"PSH  ","06-0066","纺丝机2A面VLA压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[14,"PSH  ","06-0067","纺丝机1B面VLA压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[15,"PSH  ","06-0068","纺丝机1A面VLA压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[16,"TE   ","06-0101","带套管双支铂电阻          ","PR-24UBS-75MM       ","FOXBORO US","C"," "]
[17,"PI   ","06-0102","压力表         ","#45-1279AS          ","ASHCROFT","C"," "]
[18,"PI   ","06-0106","压力表         ","#45-1279AS          ","ASHCROFT","C"," "]
[19,"TE   ","06-0107","带套管双支铂电阻        ","PR-24UBS-75MM       ","FOXBORO US","C"," "]
[20,"PI   ","06-0108","压力表           ","#45-1279AS          ","ASHCROFT","C"," "]
[21,"PI   ","06-0112","压力表        ","#45-1279AS          ","ASHCROFT","C"," "]
[22,"PI   ","06-0206","压力表        ","#45-1279AS          ","ASHCROFT","C"," "]
[23,"FN   ","06-0207","机械式批量控制器","ER-12/273","BROOKS","C"," "]
[24,"PI-A ","06-0209","压力表         ","#45-1279AS          ","ASHCROFT","C"," "]
[25,"PI-B ","06-0209","压力表         ","#45-1279AS          ","ASHCROFT","C"," "]
[27,"TE   ","06-0214","带套管双支铂电阻        ","PR-24UBS-225MM      ","FOXBORO US","C"," "]
[28,"PI   ","06-0219","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[32,"PSL  ","06-0225","压力开关        ","PPDN7KKT06          ","ASHCROFT","C"," "]
[33,"TE   ","06-0227","带套管双支铂电阻        ","PR-24UBS","FOXBORO US","C"," "]
[36,"FI   ","06-0234","流量计","1110, SIZE 8        ","BROOKS","C"," "]
[37,"FI   ","06-0235","流量计","1110, SIZE 8        ","BROOKS","C"," "]
[38,"PSL  ","06-0238","压力开关        ","PPDN7KKT06          ","ASHCROFT","C"," "]
[40,"TE   ","06-0302","温包    ","45P-F5","FOXBORO US","C"," "]
[41,"TE   ","06-0306","温包","45P-F5","FOXBORO US","C"," "]
[42,"TE   ","06-0308","温包    ","45P-F5","FOXBORO US","C"," "]
[43,"TT   ","06-0312","温度变送器","3144P","ROSEMOUNT","C"," "]
[48,"PSH  ","06-0315","压力开关       ","PPDN7KKT06          ","ASHCROFT","C"," "]
[49,"PSH  ","06-0316","压力开关       ","PPDN7KKT06          ","ASHCROFT","C"," "]
[50,"PSH  ","06-0317","压力开关        ","PPDN7KKT06          ","ASHCROFT","C"," "]
[51,"PSH  ","06-0318","压力开关       ","PPDN7KKT06          ","ASHCROFT","C"," "]
[56,"TI","06-2001","4#纺丝机热水温度双金属温度计",null,"ASHCROFT","C"," "]
[57,"PI","06-2010A","纺丝机4B侧VAL压力表","40GD20WM","WIKA","C"," "]
[58,"PI","06-2010B","纺丝机4B侧VAL压力表","40GD21WM","WIKA","C"," "]
[59,"PI","06-2024A","纺丝机4A侧VAL压力表","40GD22WM","WIKA","C"," "]
[60,"PI","06-2024B","纺丝机4A侧VAL压力表","40GD23WM","WIKA","C"," "]
[61,"TI","06-2034","3#纺丝机热水温度双金属温度计",null,"ASHCROFT","C"," "]
[62,"PI","06-2043A","纺丝机3A侧VAL压力表",null,"WIKA","C"," "]
[63,"PI","06-2043B","纺丝机3A侧VAL压力表",null,"WIKA","C"," "]
[64,"PI","06-2057A","纺丝机3B侧VAL压力表",null,"WIKA","C"," "]
[65,"PI","06-2057B","纺丝机3B侧VAL压力表",null,"WIKA","C"," "]
[66,"PSH","06-2065","纺丝机4B面VLA压力开关",null,"ASHCROFT","C"," "]
[67,"PSH","06-2066","纺丝机4A面VLA压力开关",null,"ASHCROFT","C"," "]
[68,"PSH","06-2067","纺丝机3B面VLA压力开关",null,"ASHCROFT","C"," "]
[69,"PSH","06-2068","纺丝机3A面VLA压力开关",null,"ASHCROFT","C"," "]
[70,"TT","06-2101","4#纺丝机预热水温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0075D0075T44","ROSEMOUNT","C"," "]
[71,"PI","06-2102","CONDENSATE HEADER PRESSURE AT METIER NO.4压力表         "," ","WIKA","C"," "]
[72,"PI","06-2106","METIER 4 热水泵出口压力表"," ","WIKA","C"," "]
[73,"TT","06-2107","3#纺丝机预热水温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0075D0075T44","ROSEMOUNT","C"," "]
[74,"PI","06-2108","CONDENSATE PRESSURE AT METIER NO.3 HOT W 压力表            "," ","WIKA","C"," "]
[75,"PI","06-2112","METIER 3 热水泵出口压力表"," ","WIKA","C"," "]
[76,"LT","06-2201","ST-90返回排气槽液位变送器","3301HA1S1E5AM0300RAI5M1Q4","ROSEMOUNT","C"," "]
[77,"PI","06-2209A","ST-90 RETURN PUMP DOWNSTREAM STRAINER PRES 压力表     ",null,"WIKA","C"," "]
[78,"PI","06-2209B","ST-90 RETURN PUMP UPSTREAM STRAINER PRES 压力表   ",null,"WIKA","C"," "]
[79,"FT","06-2210","卷曲机压缩空气总管流量涡街流量计",null,"ROSEMOUNT","C"," "]
[81,"PdI","06-2231","DI FEED WATER TO TOW CRIMPERS 13-18压差表 "," ","ASHCROFT","C"," "]
[83,"PdI","06-2232","DI FEED WATER TO TOW CRIMPERS 19-24压差指示"," ","ASHCROFT","C"," "]
[85,"FI","06-2234","ST-90至3#纺丝机转子流量计  ","1/2 INCH FULL VIEW FLOWME","科隆","C"," "]
[86,"FI","06-2235","ST-90至4#纺丝机转子流量计","1/2 INCH FULL VIEW FLOWME","科隆","C"," "]
[87,"TT","06-2302","纺丝机6A面VLA排气管温度","3144PD1A2I5B4M5Q4/0065D22D0035D0300T44","ROSEMOUNT","C"," "]
[88,"TT","06-2306","纺丝机4B面VLA排气管温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0300T44","ROSEMOUNT","C"," "]
[89,"TT","06-2308","纺丝机3A面VLA排气管温度","3144PD1A2I5B4M5Q4/0065D22D0035D0300T44","ROSEMOUNT","C"," "]
[90,"TT","06-2312","纺丝机3B面VLA排气管温度","3144PD1A2I5B4M5Q4/0065D22D0035D0300T44","ROSEMOUNT","C"," "]
[91,"PSH","06-2313","纺丝机4A面排气管压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[92,"PT","06-2313A","纺丝机3A面VAL排气管压力差压变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," "]
[93,"PT","06-2313B","纺丝机3B面VAL排气管压力差压变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," "]
[94,"PSH","06-2314","纺丝机4B面排气管压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[95,"PSH","06-2315","纺丝机3A面排气管压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[96,"PSH","06-2316","纺丝机3B面排气管压力开关","PPDN7KKT06          ","ASHCROFT","C"," "]
[97,"FT","06-2321","3#纺丝机A面排气流量一体化流量变送器","3051SFADG360ZCUFS2A1B0031AA1A2M5","ROSEMOUNT","C"," "]
[98,"FT","06-2322","3#纺丝机B面排气流量一体化流量变送器","3051SFADG360ZCUFS2A1B0031AA1A2M5","ROSEMOUNT","C"," "]
[99,"FT","06-2323","4#纺丝机A面排气流量一体化流量变送器","3051SFADG360ZCUFS2A1B0031AA1A2M5","ROSEMOUNT","C"," "]
[100,"FT","06-2324","4#纺丝机B面排气流量一体化流量变送器","3051SFADG360ZCUFS2A1B0031AA1A2M5","ROSEMOUNT","C"," "]
[101,"FI","06-401","1#纺丝机热水供给流量转子流量计 ",null,"科隆","C"," "]
[102,"FI","06-402","2#纺丝机热水供给流量转子流量计"," ","科隆","C"," "]
[103,"FI","07-0005","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[104,"FI","07-0006","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[105,"FI","07-0007","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[106,"FI","07-0008","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[107,"FI","07-0013","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[108,"FI","07-0014","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[109,"FI","07-0015","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[110,"FI","07-0016","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[111,"PT","07-002","1A1压板压力变送器","IGP10","FOXBORO","C"," "]
[112,"FI","07-0021","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[113,"FI","07-0022","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[114,"FI","07-0023","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[115,"FI","07-0024","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[116,"PT","07-003","1A1雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[117,"PIT","07-004","1A1对辊压力变送器","IGP10","FOXBORO","C"," "]
[118,"PIT","07-010","1A2压板压力变送器","IGP10","FOXBORO","C"," "]
[119,"FI","07-0105","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[120,"FI","07-0106","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[121,"FI","07-0107","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[122,"FI","07-0108","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[123,"PIT","07-011","1A2雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[124,"FI","07-0113","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[125,"FI","07-0114","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[126,"FI","07-0115","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[127,"FI","07-0116","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[128,"PIT","07-012","1A2对辊压力变送器","IGP10","FOXBORO","C"," "]
[129,"FI","07-0121","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[130,"FI","07-0122","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[131,"FI","07-0123","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[132,"FI","07-0124","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[134,"PI   ","07-0128","压力表        ","#45-1279AS          ","ASHCROFT","C"," "]
[135,"FT   ","07-0130","流量变送器        ","ST98","FCI FLUID           ","C"," "]
[136,"TT","07-0131","温度变送器","3144P","ROSEMOUNT","C"," "]
[137,"TT","07-0137","温度变送器","3145P","ROSEMOUNT","C"," "]
[138,"TT","07-0150","温度变送器","3146P","ROSEMOUNT","C"," "]
[139,"PID","07-0153","差压计","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[140,"PIT","07-018","1A3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[141,"PIT","07-019","1A3雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[142,"PIT","07-020","1A3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[143,"FI","07-0205","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[144,"FI","07-0206","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[145,"FI","07-0207","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[146,"FI","07-0208","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[147,"FI","07-0213","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[148,"FI","07-0214","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[149,"FI","07-0215","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[150,"FI","07-0216","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[151,"FI","07-0221","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[152,"FI","07-0222","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[153,"FI","07-0223","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[154,"FI","07-0224","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[156,"PI   ","07-0228","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[157,"FT   ","07-0230","流量变送器        ","ST98","FCI FLUID           ","C"," "]
[158,"TT","07-0231","温度变送器","3144P","ROSEMOUNT","C"," "]
[159,"TT","07-0237","温度变送器","3145P","ROSEMOUNT","C"," "]
[160,"TT","07-0250","温度变送器","3146P","ROSEMOUNT","C"," "]
[161,"PID","07-0253","差压计","40GD10WM","MERIAM INSTRUMENT   ","C"," "]
[162,"FI","07-0305","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[163,"FI","07-0306","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[164,"FI","07-0307","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[165,"FI","07-0308","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[166,"FI","07-0313","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[167,"FI","07-0314","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[168,"FI","07-0315","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[169,"FI","07-0316","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[170,"FI","07-0321","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[171,"FI","07-0322","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[172,"FI","07-0323","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[173,"FI","07-0324","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[174,"PT","07-102","1B1压板压力压力变送器","IGP10","FOXBORO","C"," "]
[175,"PT","07-103","1B1雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[176,"PT","07-104","1B1对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[177,"PT","07-110","1B2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[178,"PT","07-111","1B2雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[179,"PT","07-112","1B2对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[180,"PT","07-118","1B3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[181,"PT","07-119","1B3雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[182,"PT","07-120","1B3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[183,"PT","07-2002","3A1压板压力变送器","IGP10","FOXBORO","C"," "]
[184,"PT","07-2003","3A1雾化水压力表","IGP10","FOXBORO","C"," "]
[185,"PIT","07-2004","1A1对辊压力变送器","IGP10","FOXBORO","C"," "]
[186,"FI","07-2005","3A1对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[187,"FI","07-2006","3A1对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[188,"FI","07-2007","3A1对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[189,"FI","07-2008","3A1对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[190,"PIT","07-2010","3A2压板压力变送器","IGP10","FOXBORO","C"," "]
[191,"PIT","07-2011","3A2雾化水压力表","IGP10","FOXBORO","C"," "]
[192,"PIT","07-2012","3A2对辊压力变送器","IGP10","FOXBORO","C"," "]
[193,"FI","07-2013","3A2对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[194,"FI","07-2014","3A2对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[195,"FI","07-2015","3A2对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[196,"FI","07-2016","3A2对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[197,"PIT","07-2018","3A3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[198,"PIT","07-2019","3A3雾化水压力表","IGP10","FOXBORO","C"," "]
[199,"PT","07-202","2A1压板压力变送器","IGP10","FOXBORO","C"," "]
[200,"PIT","07-2020","3A3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[201,"FI","07-2021","3A3对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[202,"FI","07-2022","3A3对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[203,"FI","07-2023","3A3对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[204,"FI","07-2024","3A3对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[205,"PT","07-203","2A1雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[206,"PIT","07-204","2A1对辊压力变送器","IGP10","FOXBORO","C"," "]
[207,"PIT","07-210","2A2压板压力变送器","IGP10","FOXBORO","C"," "]
[208,"PT","07-2102","3B2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[209,"PT","07-2103","3B1雾化水压力表","IGP10","FOXBORO","C"," "]
[210,"PT","07-2104","3B1对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[211,"FI","07-2105","3B1对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[212,"FI","07-2106","3B1对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[213,"FI","07-2107","3B1对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[214,"FI","07-2108","3B1对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[215,"PIT","07-211","2A2雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[216,"PT","07-2110","3B2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[217,"PT","07-2111","3B2雾化水压力表","IGP10","FOXBORO","C"," "]
[218,"PT","07-2112","3B2对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[219,"FI","07-2113","3B2对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[220,"FI","07-2114","3B2对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[221,"FI","07-2115","3B2对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[222,"FI","07-2116","3B2对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[223,"PT","07-2118","3B3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[224,"PT","07-2119","3B3雾化水压力表","IGP10","FOXBORO","C"," "]
[225,"PIT","07-212","2A2对辊压力变送器","IGP10","FOXBORO","C"," "]
[226,"PT","07-2120","3B3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[227,"FI","07-2121","3B3对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[228,"FI","07-2122","3B3对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[229,"FI","07-2123","3B3对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[230,"FI","07-2124","3B3对辊下右喷嘴冷却水流量","A6131B053INA0AAS","ABB","C"," "]
[231,"FT","07-2127","3#干燥机喷雾蒸汽流量流量计","1195S010A1S0630CS4","ROSEMOUNT","C"," "]
[232,"PI","07-2128","DRYER NO.4 STEAM SUPPLY 压力表       ","           ","WIKA","C"," "]
[233,"FT","07-2130","3#干燥机排气流量一体化流量变送器","3051SFADG200ZCHPS2T100031AA1A2RLM5","ROSEMOUNT","C"," "]
[234,"TT","07-2131","3#干燥机1区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[235,"FSL","07-2133","3#干燥机1区循环空气低流量流量开关",null,"FCI","C"," "]
[236,"FSL","07-2136","3#干燥机2区循环空气低流量流量开关",null,"FCI","C"," "]
[237,"TT","07-2137","3#干燥机2区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[238,"FSL","07-2139","3#干燥机3区循环空气低流量流量开关",null,"FCI","C"," "]
[239,"TT","07-2150","3#干燥机3区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[240,"PDI","07-2153","STREAM 32A TO VLA SYSTEM差压表 ",null,"ASHCROFT","C"," "]
[241,"FSL","07-2156","3#干燥机4区循环空气低流量流量开关",null,"FCI","C"," "]
[242,"PIT","07-218","2A3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[243,"PIT","07-219","2A3雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[244,"PIT","07-220","2A3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[245,"PT","07-2202","4A1压板压力压力变送器","IGP10","FOXBORO","C"," "]
[246,"PT","07-2203","4A1雾化水压力表","IGP10","FOXBORO","C"," "]
[247,"PT","07-2204","4A1对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[248,"FI","07-2205","4A1对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[249,"FI","07-2206","4A1对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[250,"FI","07-2207","4A1对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[251,"FI","07-2208","4A1对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[252,"PT","07-2210","4A2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[253,"PT","07-2211","4A2雾化水压力变送器","IGP10","FOXBORO","C"," "]
[254,"PT","07-2212","4A2对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[255,"FI","07-2213","4A2对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[256,"FI","07-2214","4A2对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[257,"FI","07-2215","4A2对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[258,"FI","07-2216","4A2对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[259,"PT","07-2218","4A3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[260,"PT","07-2219","4A3雾化水压力表","IGP10","FOXBORO","C"," "]
[261,"PT","07-2220","4A3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[262,"FI","07-2221","4A3对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[263,"FI","07-2222","4A3对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[264,"FI","07-2223","4A3对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[265,"FI","07-2224","4A3对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[266,"FT","07-2227","4#干燥机喷雾蒸汽流量流量计","1195S010A1S0630CS4","ROSEMOUNT","C"," "]
[267,"PI","07-2228","DRYER NO.4 STEAM SUPPLY 压力表       "," ","WIKA","C"," "]
[268,"FT","07-2230","4＃干燥机排气流量一体化流量变送器","3051SFADG200ZCHPS2T100031AA1A2RLM5","ROSEMOUNT","C"," "]
[269,"TT","07-2231","4#干燥机1区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[270,"FSL","07-2236","4#干燥机2区循环空气低流量流量开关",null,"FCI","C"," "]
[271,"TT","07-2237","4#干燥机2区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[272,"FSL","07-2239","4＃干燥机3区循环空气低流量流量开关",null,"FCI","C"," "]
[273,"TT","07-2250","4#干燥机3区温度一体化温度变送器     ","3144PD1A2I5B4M5U6Q4","ROSEMOUNT","C"," "]
[274,"PDI","07-2253","STREAM 32A TO VLA SYSTEM差压表 "," ","ASHCROFT","C"," "]
[275,"FSL","07-2256","4＃干燥机4区循环空气低流量流量开关"," ","FCI","C"," "]
[276,"PT","07-2302","4B1压板压力压力变送器","IGP10","FOXBORO","C"," "]
[277,"PT","07-2303","4B1雾化水压力表","IGP10","FOXBORO","C"," "]
[278,"PT","07-2304","4B1对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[279,"FI","07-2305","4B1对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[280,"FI","07-2306","4B1对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[281,"FI","07-2307","4B1对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[282,"FI","07-2308","4B1对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[283,"PT","07-2310","4B2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[284,"PT","07-2311","4B2雾化水压力表","IGP10","FOXBORO","C"," "]
[285,"PT","07-2312","4B2对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[286,"FI","07-2313","4B2对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[287,"FI","07-2314","4B2对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[288,"FI","07-2315","4B2对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[289,"FI","07-2316","4B2对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[290,"PT","07-2318","4B3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[291,"PT","07-2319","4B3雾化水压力表","IGP10","FOXBORO","C"," "]
[292,"PT","07-2320","4B3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[293,"FI","07-2321","4B3对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[294,"FI","07-2322","4B3对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[295,"FI","07-2323","4B3对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[296,"FI","07-2324","4B3对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[297,"PIT","07-3002","1A4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[298,"PIT","07-3003","1A4雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[299,"PIT","07-3004","1A4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[300,"FI","07-3005","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[301,"FI","07-3006","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[302,"FI","07-3007","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[303,"FI","07-3008","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[304,"PT","07-302","2B1压板压力压力变送器","IGP10","FOXBORO","C"," "]
[305,"PT","07-303","2B1雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[306,"PT","07-304","2B1对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[307,"PT","07-310","2B2压板压力压力变送器","IGP10","FOXBORO","C"," "]
[308,"PIT","07-3102","1B4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[309,"PIT","07-3103","1B4雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[310,"PIT","07-3104","1B4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[311,"FI","07-3105","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[312,"FI","07-3106","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[313,"FI","07-3107","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[314,"FI","07-3108","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[315,"PT","07-311","2B2雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[316,"PT","07-312","2B2对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[317,"PT","07-318","2B3压板压力压力变送器","IGP10","FOXBORO","C"," "]
[318,"PT","07-319","2B3雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[319,"PT","07-320","2B3对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[320,"PIT","07-3202","2A4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[321,"PIT","07-3203","2A4雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[322,"PIT","07-3204","2A4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[323,"FI","07-3205","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[324,"FI","07-3206","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[325,"FI","07-3207","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[326,"FI","07-3208","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[327,"PIT","07-3302","2B4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[328,"PIT","07-3303","2B4雾化水压力表","2.5kg/cm2","ASHCROFT","C"," "]
[329,"PIT","07-3304","2B4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[330,"FI","07-3305","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[331,"FI","07-3306","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[332,"FI","07-3307","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[333,"FI","07-3308","转子流量计","10A6131NB1B","Fischer & Porter","C"," "]
[334,"PIT","07-3402","3A5压板压力压力变送器","IGP10","FOXBORO","C"," "]
[335,"PIT","07-3403","3A4雾化水压力表","IGP10","FOXBORO","C"," "]
[336,"PIT","07-3404","3A5对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[337,"FI","07-3405","3A4对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[338,"FI","07-3406","3A4对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[339,"FI","07-3407","3A4对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[340,"FI","07-3408","3A4对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[341,"PIT","07-3502","3B4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[342,"PIT","07-3503","3B4雾化水压力表","IGP10","FOXBORO","C"," "]
[343,"PIT","07-3504","3B4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[344,"FI","07-3505","3B4对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[345,"FI","07-3506","3B4对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[346,"FI","07-3507","3B4对辊下左喷嘴冷却水流量转子流量计","A6131B053INA1AAS","ABB","C"," "]
[347,"FI","07-3508","3B4对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[348,"PIT","07-3602","4A4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[349,"PIT","07-3603","4A4雾化水压力表","IGP10","FOXBORO","C"," "]
[350,"PIT","07-3604","4A4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[351,"FI","07-3605","4A4对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[352,"FI","07-3606","4A4对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[353,"FI","07-3607","4A4对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[354,"FI","07-3608","4A4对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[355,"PIT","07-3702","4B4压板压力压力变送器","IGP10","FOXBORO","C"," "]
[356,"PIT","07-3703","4B4雾化水压力表","IGP10","FOXBORO","C"," "]
[357,"PIT","07-3704","4B4对辊压力压力变送器","IGP10","FOXBORO","C"," "]
[358,"FI","07-3705","4B4对辊上左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[359,"FI","07-3706","4B4对辊上右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[360,"FI","07-3707","4B4对辊下左喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[361,"FI","07-3708","4B4对辊下右喷嘴冷却水流量转子流量计","A6131B053INA0AAS","ABB","C"," "]
[362,"PI   ","08-0208","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[385,"TI   ","11-0002","温度计  ","50EI60E090          ","ASHCROFT","C"," "]
[386,"TE   ","11-0003","现场温包    ","45P-F5","FOXBORO US","C"," "]
[387,"TI   ","11-0007","温度计  ","50EI60E090          ","ASHCROFT","C"," "]
[388,"DPI  ","11-0008","差压指示仪 ","\"U\"形管","国产","C"," "]
[389,"TI   ","11-0010","温度计","50EI60E090          ","ASHCROFT","C"," "]
[390,"TE   ","11-0011","热电阻","PR-24UBS","FOXBORO US","C"," "]
[391,"TI   ","11-0015","温度计 ","50EI60E090          ","ASHCROFT","C"," "]
[392,"DPI  ","11-0016","差压指示仪 ","\"U\"形管","国产","C"," "]
[393,"PI   ","13-0603","压力表         ","#45-1279AS          ","ASHCROFT","C"," "]
[394,"PI   ","13-0604","压力表           ","#45-1279AS          ","ASHCROFT","C"," "]
[395,"PI   ","13-0613","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[396,"PI   ","13-0614","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[397,"PI   ","13-0615","压力表          ","#45-1279AS          ","ASHCROFT","C"," "]
[404,"TT","05-0011","温度变送器",null,"ROSEMOUNT","C"," "]
[414,"PI","2001","加热板供汽压力表","0-1MPa",null,"C"," "]
[46,"AIT  ","06-0314","纺丝一期丙酮分析仪     ","ULTRAMAT 6       ","SIEMENS         ","B","±1.0%",{"$nulls":4},"见校验记录","自校验"]
[47,"AIT  ","06-2314","纺丝二期丙酮分析仪     ","ULTRAMAT 6       ","SIEMENS         ","B","±1.0%",{"$nulls":4},"见校验记录","自校验"]
[398,"TI   ","13-0616","清洗槽温度计 ","0-100℃","杭州富阳仪川","C"]
[399,"TI   ","13-0617","清洗槽温度计 ","0-100℃","杭州富阳仪川","C"]
[400,"TI   ","13-0618","清洗槽温度计 ","0-100℃","杭州富阳仪川","C"]
[401,"TI   ","13-0619","清洗槽温度计 ","0-100℃","杭州富阳仪川","C"]
[405,"DPI  ","06-231","差压表",null,null,"C"]
[406,"DPI  ","06-232","差压表",null,null,"C"]
[407,"TT","11-2003","温度变速器",null,"ROSEMOUNT","C"]
[408,"TT","11-2011","温度变速器",null,"ROSEMOUNT","C"]
[411,"LG","06-215","液位计",null,null,"C"]
[412,"LG","06-216","液位计",null,null,"C"]
[413,"LG","06-217","液位计",null,null,"C"]
[415,"FT","10-016","进丝束大楼3KG蒸汽流量","3095MFAS100CCHPS2T100T32CA1ARLE5M5","ROSEMOUNT","C"]
[417,"FT","06-2310","ST-90油剂流量质量流量计","R025S116NCAAMZZZZ+1700I11ABAMZZZ","ROSEMOUNT","C"]
[418,"FT","06-2312","ST-90脱离子水流量质量流量计","R050S131NCAAMZZZZ+1700I11ABAMZZZ","ROSEMOUNT","C"]
[419,"PI","07-401","1#干燥机1#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[420,"PI","07-402","1#干燥机1#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[421,"PI","07-403","1#干燥机2#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[422,"PI","07-404","1#干燥机2#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[423,"PI","07-405","1#干燥机3#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[424,"PI","07-406","1#干燥机3#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[425,"PI","07-407","2#干燥机1#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[426,"PI","07-408","2#干燥机1#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[427,"PI","07-409","2#干燥机2#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[428,"PI","07-410","2#干燥机2#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[429,"PI","07-411","2#干燥机3#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[430,"PI","07-412","2#干燥机3#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[431,"PI","07-413","3#干燥机1#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[432,"PI","07-414","3#干燥机1#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[433,"PI","07-415","3#干燥机2#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[434,"PI","07-416","3#干燥机2#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[435,"PI","07-417","3#干燥机3#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[436,"PI","07-418","3#干燥机3#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[437,"PI","07-419","4#干燥机1#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[438,"PI","07-420","4#干燥机1#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[439,"PI","07-421","4#干燥机2#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[440,"PI","07-422","4#干燥机2#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[441,"PI","07-423","4#干燥机3#疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[442,"PI","07-424","4#干燥机3#疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[443,"PI","07-425","1#预热风机疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[444,"PI","07-426","1#预热风机疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[445,"PI","07-427","2#预热风机疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[446,"PI","07-428","2#预热风机疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[447,"PI","07-429","3#预热风机疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[448,"PI","07-430","3#预热风机疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[449,"PI","07-431","4#预热风机疏水泵入口压力表","0~2.5MPa","Spirax Sarco","C"]
[450,"PI","07-432","4#预热风机疏水泵出口压力表","0~1.0MPa","Spirax Sarco","C"]
[451,"PI","07-433","凝液回收换热器入口压力表","0~2.5MPa","Spirax Sarco","C"]
[452,"PI","07-434","凝液回收换热器集水管压力表","0~2.5MPa","Spirax Sarco","C"]
[453,"TT","07-435","凝液回收换热器入口温度变送器","0-100℃","上仪","C"]
[454,"TT","07-436","凝液回收换热器出口温度变送器","0-100℃","上仪","C"]
[16,"PT","04-0041","2&3#醋片溶解釜压力压力变送器","1151DP3S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[80,"PT","04-0327","2B溶解釜排空压力变送器","1151DP3S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[118,"PT","04-2430","废丝釜VTA压力变送器","3051S1TG3A2E11A1AB4D1I5M5Q4","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[95,"LT   ","04-0518","TIO2乳液储槽液位变送器  ","30511S1TG1A2B11A1AB4D1I5M5Q4","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[14,"PT","04-0033","1#醋片溶解釜压力压力变送器","1151DP3S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[41,"LT","04-0133","加热器储槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[55,"PT","04-0214","C级滤前压力压力变送器","1151GP7S12S1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[58,"PT","04-0217","C级滤后压力压力变送器","1151GP6S12S1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[63,"PT   ","04-0224","三级滤后压力压力变送器","1151GP7S12S1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[119,"PT","04-3217","三级滤前压力压力变送器","3051S1TG3A2B11A1AB4D1I5M5Q4","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[145,"AIT","04-0201","废丝釜氧分析仪","SERVOMEX 2200","英国","B",{"$nulls":5},"见校验记录","自校验"]
[1,"FI   ","03-008","流量计         ","1110, SIZE 8                ","BROOKS              ","C"," "]
[2,"FI   ","04-0009","流量计 ","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[3,"FI   ","04-0011","进入1#溶解釜的氮气转子流量计","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[4,"TI   ","04-0012","温度计","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[5,"TI   ","04-0018","温度计","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[6,"FI   ","04-0021","进入3#溶解釜的氮气转子流量计","1110, SIZE 7        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[7,"TI   ","04-0022","温度计","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[8,"LT","04-0024","3#溶解釜液位变送器","1151LT4SA0H22D15","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[9,"TE   ","04-0025","带套管双支铂电阻    ","PR-24UBS-225MM      ","FOXBORO US            ","C"," ",{"$nulls":3}," "]
[10,"PI   ","04-0028","压力表       ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[11,"PI   ","04-0029","压力表          ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[12,"FT   ","04-0030","涡街        ","83F-A-01S1SSTNJ","FOXBORO US            ","C"," ",{"$nulls":3}," "]
[13,"FI   ","04-0031","进入2#溶解釜的氮气转子流量计","1110, SIZE 7        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[15,"PI   ","04-0039","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[17,"PT","04-0042","未过滤浆液压力变送器","1151GP6S12S1I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[18,"FI   ","04-0051","进入1#溶解釜醋片进口的氮气转子流量计","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[19,"FI   ","04-0052","流量计  ","1110, SIZE 6        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[20,"LT","04-0101","1#A-贮罐液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[23,"LT","04-0105","2#A-贮罐液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[24,"PI   ","04-0108","压力表        ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[25,"PI   ","04-0111","压力表   ","#45-1279AS  2.5MPa     ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[26,"TI   ","04-0112","温度计","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[27,"PI   ","04-0113A","压力表        ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[28,"PI","04-0113B","压力表        ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[29,"PI","04-0118","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[30,"TE","04-0119","带套管双支铂电阻","PR-24UBS-100MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[31,"PI","04-0120","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[32,"TI","04-0121","温度计","50EI60E060","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[33,"PI","04-0122","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[34,"TI","04-0123","温度计","50EI60E060","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[35,"PI","04-0124","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[36,"PI","04-0125","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[37,"PI","04-0127","压力表","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[38,"TI","04-0130","温度计","50EI60E090          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[39,"TE","04-0131","带套管双支铂电阻","PR-24UBS-050MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[40,"PI","04-0132","压力表","#45-1279AS 4Kg","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[42,"PT   ","04-0201","A级滤前压力压力变送器","1151GP7S12S1I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[43,"PI   ","04-0202","压力表         ","#45-1279AS  2.5MPa     ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[44,"DPT","04-0203","压力变送器（1#CROFT）","1151DP8S","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[45,"PI","04-0203A","压力表  ","#45-1280AS","ASHCROFT","C"," ",{"$nulls":3}," "]
[46,"PI","04-0203B","压力表  ","#45-1281AS","ASHCROFT","C"," ",{"$nulls":3}," "]
[47,"PT","04-0204","A级滤后压力压力变送器","1151GP6S12S1I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[48,"LT","04-0205","C-贮槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[50,"PI   ","04-0207","压力表      ","#45-1279AS  1MPa","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[51,"WIT","04-0208","二楼平台称","H90-3051","FAIRBANK","C"," ",{"$nulls":3}," "]
[52,"PI   ","04-0209","压力表        ","#45-1279AS  2.5MPa     ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[53,"PI","04-0211","2级过滤出口压力表","0~2.5MPa","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[54,"PSHL ","04-0213","压力开关      ","PPDN7KKT06          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[56,"PI","04-0215","压力表  ","0~2.5MPa","青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[57,"PI","04-0216","压力表  ","0~2.5MPa","青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[59,"PI","04-0221","压力表  ","0~2.5MPa","青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[60,"DPT","04-0222","压力变送器（2#CROFT）","1151DP8S","ROSEMOUNT","C"," "]
[61,"PI","04-0222A","压力表  ","#45-1282AS","ASHCROFT","C"," ",{"$nulls":3}," "]
[62,"PI","04-0222B","压力表  ","#45-1282AS","ASHCROFT","C"," ",{"$nulls":3}," "]
[64,"TE   ","04-0225","带套管双支铂电阻        ","PR-24UBS-100MM      ","FOXBORO US","C"," ",{"$nulls":3}," "]
[65,"PI   ","04-0226","压力表         ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[66,"TE   ","04-0227","带套管双支铂电阻            ","PR-24UBS-100MM      ","FOXBORO US            ","C"," ",{"$nulls":3}," "]
[67,"PSL  ","04-0228","压力开关     ","PPDN7KKT06          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[68,"PI   ","04-0229","压力表        ","#45-1279AS  2.5MPa    ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[69,"PI","04-0231","压力表        ","0~2.5MPa"," 青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[70,"FT   ","04-0302","涡街        ","83F-A-1HS1SSTNJ","FOXBORO US","C"," ",{"$nulls":3}," "]
[71,"TI   ","04-0306","温度计  ","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[72,"PI   ","04-0308","压力表      ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[73,"PI   ","04-0310","压力表       ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[74,"FI   ","04-0311","流量计  ","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[75,"PI   ","04-0313","压力表       ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[76,"LT   ","04-0314","3#A-贮槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[78,"PI-A ","04-0317","压力表         ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[79,"PI-B ","04-0317","压力表     ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[81,"FI   ","04-0328","进入2B#溶解釜的氮气转子流量计","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[82,"FI   ","04-0329","流量计    ","1110, SIZE 8        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[83,"PI   ","04-0401","压力表     ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[84,"PI   ","04-0403","压力表   ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[85,"PI   ","04-0405","压力表         ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[86,"TI","04-0405","温度计","50EI60E120","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[87,"LT","04-0408","脏丙酮储槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[88,"LT","04-0411","清洁丙酮储槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[89,"PI   ","04-0412","压力表    ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[91,"FI   ","04-0415","流量计    ","1110, SIZE 7        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[92,"PI   ","04-0509","压力表     ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[93,"PI   ","04-0512","压力表   ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[94,"PI   ","04-0514","压力表       ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[96,"PI   ","04-0519","压力表       ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[97,"LT   ","04-0521","超声波液位计      ",null,"SIEMENS","C"," ",{"$nulls":3}," "]
[98,"PI   ","04-0523","压力表     ","#45-1279AS          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[99,"PSH  ","04-0523","压力开关    ","PPDN7KKT06          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[100,"TI   ","04-0527","温度计","50E160E120          ","ASHCROFT            ","C"," ",{"$nulls":3}," "]
[101,"FM   ","04-0529","机械式批量计     ","9453FB7C1A2A        ","BROOKS              ","C"," ",{"$nulls":3}," "]
[102,"FI","04-2021","进入4#溶解釜的氮气转子流量计",null,"科隆","C"," ",{"$nulls":3}," "]
[103,"LT","04-2024","4#溶解釜液位计","3051S1LD2AA1A1010DFFJGDA00D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[104,"TT","04-2025","4#溶解釜温度变送器","3144PD1A2I5B4M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[105,"PI","04-2028","4#溶解釜泵04-210.00的入口压力表","","WIKA","C"," ",{"$nulls":3}," "]
[106,"FT","04-2035","1#和2＃溶解釜工艺水流量质量流量计","CMF025M300NQBUMZZZ+1700R11ABUMZZZ","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[107,"PT","04-2041","4#醋片溶解釜压力压力变送器","3051S1CD1A2B12A1AB4D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[108,"PdT","04-2203","二级滤后CRAFT差压差压变送器","3051S1CD5A2B12A1AB4D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[109,"PI","04-2203A","二级CRAFT前压力指示压力表",null,"WIKA","C"," ",{"$nulls":3}," "]
[110,"PI","04-2203B","二级CRAFT后压力指示压力表",null,"WIKA","C"," ",{"$nulls":3}," "]
[111,"TT","04-2225","二级滤后浆液温度一体化温度变送器","3144PD1A2I5B4M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[112,"LT","04-2352","2B#溶解釜液位变送器"," ","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[113,"TI","04-2414","04-203A.00废丝溶解釜温度"," ","ASHCROFT","C"," ",{"$nulls":3}," "]
[114,"LT","04-2415","04-203A.00废丝溶解釜液位"," ","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[115,"TI","04-2419","04-203B.00废丝溶解釜温度"," ","ASHCROFT","C"," ",{"$nulls":3}," "]
[116,"LT","04-2420","04-203B.00废丝溶解釜液位"," ","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[117,"FI","04-2423","进入04-203A/B.00的氮气"," ","KROHNE","C"," ",{"$nulls":3}," "]
[120,"PI","04-P1","#1釜减速箱油压","0~0.1MPa","JOHNSON","C"," ",{"$nulls":3}," "]
[121,"PI","04-P2","#2釜减速箱油压","0~0.1MPa","杭州华通","C"," ",{"$nulls":3}," "]
[122,"PI","04-P3","#3釜减速箱油压","0~0.1MPa","杭州华通","C"," ",{"$nulls":3}," "]
[123,"PI","04-P4","#R釜减速箱油压","0~0.1MPa","杭州华通","C"," ",{"$nulls":3}," "]
[124,"FSL","04-017","矿物油流量开关",null,"FCI","C"," ",{"$nulls":3}," "]
[125,"TT","04-012","温度变送器",null,"罗斯蒙特","C"]
[126,"TT","04-018","温度变送器",null,"罗斯蒙特","C"]
[127,"TT","04-025","温度变送器",null,"罗斯蒙特","C"]
[128,"TT","04-131","温度变送器",null,"罗斯蒙特","C"]
[129,"TT","04-2025","温度变送器",null,"罗斯蒙特","C"]
[130,"TT","04-2119","温度变送器",null,"罗斯蒙特","C"]
[131,"TT","04-2225","温度变送器",null,"罗斯蒙特","C"]
[132,"TT","04-225","温度变送器",null,"罗斯蒙特","C"]
[133,"TT","04-227","温度变送器",null,"罗斯蒙特","C"]
[134,"TT","04-306","温度变送器",null,"罗斯蒙特","C"]
[135,"MTT","04-450","废丝釜区域温湿度变送器",null,"VAISALA","C"]
[136,"TE"," 05-0011","铂电阻",null," ","C"]
[137,"TT"," 05-0011","温度变送器",null,"罗斯蒙特","C"]
[138,"FT","04-2609","214#空调3KG蒸汽流量","3095MFAS060CCHPS2T100T31CA1ARLE5M5","ROSEMOUNT","C"]
[139,"FT","04-0030","进2B溶解釜丙酮流量","83F-A-1HS2SSTNJ","FOXBORO ","C"]
[140,"FT","04-0032","进1#溶解釜丙酮流量质量流量计","CMF025M313NU+RFT9739E5SUK","ROSEMOUNT","C"]
[141,"FT","04-0302","进2#溶解釜丙酮流量","83F-A-1HS1SSTNJ","FOXBORO ","C"]
[142,"FT","04-2432","进废丝溶解釜丙酮流量","P95S010A1S0800CD7AA1K5Q40","ROSEMOUNT","C"]
[143,"TMT","04-15","废丝溶解釜旁温湿度变送器","HMT363","VAISALA","C"]
[287,"FT","17-0210","仪表用空气流量变送器","1151DP4S12I5,0~0.883kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[292,"FT","17-0405","冷却水供水流量变送器","1151DP4S12I5,0~7.86kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[293,"FT","17-0513","冷冻水供水流量变送器","1151DP4S12I5,0~1.33kPa ","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[297,"FT","17-0607","工艺水供水流量变送器","1151DP4S12I5,0~4.206kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[47,"FT","10-0209","进4#吸附床蒸汽流量变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[276,"PT","17-0015","3KG蒸汽压力变送器","1151GP7S22B3I5,0~588.39kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[32,"FT","10-0134","3#吸附床的VLA流量变送器","3051CD2A22A1AB1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[114,"LT","10-0700","1#原料丙酮贮槽液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[117,"LT","10-0710","2#原料丙酮贮槽液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[108,"LT","10-0502","蒸发炉冷凝液储槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[284,"FT","17-0039","10KG蒸汽流量变送器       ","1151DP4S12I5,0~3.53kPa","ROSEMOUNT","C",{"v":1,"d":"1.0"},{"$nulls":4}," "]
[20,"FT","10-0102","1#吸附床的VLA流量变送器","3051CD2A22A1AB1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[21,"FT","10-0110","进1#吸附床蒸汽流量变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[26,"FT","10-0118","2#吸附床的VLA流量变送器","3051CD2A22A1AB1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[27,"FT","10-0126","进2#吸附床蒸汽流量变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[46,"FT","10-0201","4#吸附床的VLA流量变送器","3051CD2A22A1AB1I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[285,"PT","17-0039","10KG蒸汽压力变送器","1151GP7S22B3I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[288,"PT","17-0211","仪表用空气压力变送器","1151GP7S22B3I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[291,"PT","17-0312","供氮压力变送器","1151GP7S22B3I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[290,"FT","17-0311","供氮流量变送器","3051CD1A52A1A","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[24,"PT","10-0114","1#吸附床压力变送器","1151DP5S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[30,"PT","10-0130","2#吸附床压力变送器","1151DP5S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[36,"PT","10-0146","3#吸附床压力变送器","1151DP5S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[50,"PT","10-0213","4#吸附床压力变送器","1151DP5S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[94,"LT","10-0406","1#回收丙酮贮罐液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[97,"LT","10-0410","2#回收丙酮贮罐液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[100,"LT","10-0414","3#不合格丙酮贮罐液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[102,"LT","10-0416","4#回收丙酮供应罐液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[120,"LT","10-0740","碱液贮槽液位变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[309,"LT","10-3001","热水回收槽液位变送器","3051S1CD2A2E12A1AB4D1D2I5M5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[61,"LT","10-0257","1#稀碱贮罐液位变送器","1151LT5SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[80,"LT","10-0328","1#回流槽液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[84,"LT","10-0332","1#MEO贮槽液位变送器","1151LT4SGOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[283,"LT","17-0036","冷凝水集液槽液位变送器","1151DP4S","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[107,"FT","10-0422","不合格槽到稀丙酮槽流量变送器","1151DP3S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[33,"FT","10-0142","进3#吸附床蒸汽流量变送器","1151DP4S22I5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[69,"LT","10-0311","1#精馏塔釜液位变送器","1151LT4SAOT22DI5","ROSEMOUNT","C",{"v":1,"d":"1.0"}]
[79,"FT","10-0324","1#精馏塔蒸汽流量变送器","1151DP4S22I5","ROSEMOUNT","B",{"v":1,"d":"1.0"},{"$nulls":3},"十四冶云南安装公司"]
[70,"PT","10-0312","1#精馏塔釜底压力变送器","3051S2TG3A2B11A1AB4M5","ROSEMOUNT","C"]
[1,"AIT","10-0002","VLA总管浓度丙酮分析仪","ULTRAMAT 6      ","MSA","B","±1.0%",{"$nulls":4},"见校验记录","自校验"]
[52,"AIT","10-0234","1#-5#吸附床丙酮浓度分析仪","NGA2000","ROSEMOUNT","B","±1.0%",{"$nulls":4},"见校验记录","自校验"]
[223,"AIT","10-2234","6#-10#吸附床丙酮浓度分析仪","NGA2000","Beckman Ind","B","±1.0%",{"$nulls":4},"见校验记录","自校验"]
[3,"TI","10-0015","温度计","50EI60E-240-XNH","ASHCROFT","C"," "]
[4,"PDI","10-0016","差压计","200","ITT BARTON","C"," "]
[5,"TI ","10-0017","温度计","50EI60E-180-XNH","ASHCROFT","C"," "]
[6,"PDI","10-0027","差压计","201","ITT BARTON","C"," "]
[7,"TE","10-0028","RTD","PT100","国产","C"," "]
[8,"TT","10-0028","温度变送器","STT350","HONEYWELL","C"," "]
[10,"PDI","10-0035","差压计","200","ITT BARTON","C"," "]
[11,"TI","10-0036","温度计","50EI60E-180-XNH","ASHCROFT","C"," "]
[12,"PDI","10-0046","差压计","202","ITT BARTON","C"," "]
[13,"TE","10-0047","RTD","PT100","国产","C"," "]
[14,"TT","10-0047","温度变送器","RTT20","FOXBORO US","C"," "]
[15,"PDI","10-0052","差压计","200","ITT BARTON","C"," "]
[16,"TI","10-0053","温度计","50EI60E-180-XNH","ASHCROFT","C"," "]
[17,"PDI","10-0063","差压计","203","ITT BARTON","C"," "]
[18,"TE","10-0064","RTD","PT100","国产","C"," "]
[19,"TT","10-0064","温度变送器","STT350","HONEYWELL","C"," "]
[22,"TET","10-0112","温包","45P-F5","FOXBORO US","C"," "]
[23,"TE","10-0113","热电阻","PR-24UBS-525MM","FOXBORO US","C"," "]
[25,"PDI","10-0116","差压计","227","ITT BARTON","C"," "]
[28,"TET","10-0128","温包","45P-F5","FOXBORO US","C"," "]
[29,"TE","10-0129","热电阻","PR-24UBS-525MM","FOXBORO US","C"," "]
[31,"PDI","10-0132","差压计","227","ITT BARTON","C"," "]
[34,"TET","10-0144","温包","45P-F5","FOXBORO US","C"," "]
[35,"TE","10-0145","热电阻","PR-24UBS-525MM","FOXBORO US","C"," "]
[37,"PDI","10-0148","差压计","227","ITT BARTON","C"," "]
[38,"TI","10-0151","温度计","50EI60E-40-XNH","ASHCROFT","C"," "]
[39,"TE","10-0152","热电阻","PR-24UBS-125MM","FOXBORO US","C"," "]
[40,"TI","10-0154","温度计","50EI60E-40-XNH","ASHCROFT","C"," "]
[41,"TE","10-0155","热电阻","PR-24UBS-125MM","FOXBORO US","C"," "]
[42,"TI","10-0157","温度计","50EI60E-40-XNH","ASHCROFT","C"," "]
[43,"TE","10-0158","热电阻","PR-24UBS-125MM","FOXBORO US","C"," "]
[44,"TE","10-0159","热电阻","PR-24UBS-150MM","FOXBORO US","C"," "]
[45,"FI","10-0161","转子流量计","1110CK42CMDAA","BROOKS","C"," "]
[48,"TET","10-0211","温包","45P-F5","FOXBORO US","C"," "]
[49,"TE","10-0212","热电阻","PR-24UBS-525MM","FOXBORO US","C"," "]
[51,"PDI","10-0215","差压计","227","ITT BARTON","C"," "]
[53,"LT","10-0237","1#吸附床集液槽液位变送器","3051","ROSEMOUNT","C"," "]
[54,"LT","10-0242","1#稀丙酮槽液位变送器","3051S1LD2AA1A1010DFFJGDA00D1I5M5Q4","ROSEMOUNT","C"," "]
[55,"LT","10-0244","2#稀丙酮槽液位变送器","3051S1LD2AA1A1010DFFJGDA00D1I5M5Q4","ROSEMOUNT","C"," "]
[56,"PI","10-0246","压力表","45-1279ASL-04L-XNH 1Mp","ASHCROFT","C"," "]
[57,"PI","10-0248","压力表","45-1279ASL-04L-XNH 1Mp","ASHCROFT","C"," "]
[58,"FT","10-0250","进1#精馏塔稀丙酮流量质量流量计","F025SI113SU+IFT970116D3U","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[59,"PI","10-0255","压力表","45-1279AS-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[60,"PDI","10-0256","差压计","227","ITT BARTON","C"," ",{"$nulls":3}," "]
[63,"TE","10-0301","热电阻","PR-24UBS-50MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[64,"PI","10-0304","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[65,"PI","10-0305","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[66,"PI","10-0307","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[67,"FI","10-0308","转子流量计","3633A07B2A1A","BROOKS","C"," ",{"$nulls":3}," "]
[68,"TI","10-0310","温度计","50EI60E-40-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[71,"TE","10-0313","热电阻","PR-24UBS-325MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[72,"TE","10-0314","热电阻","PR-24UBS-325MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[73,"FI ","10-0316","转子流量计","1110CK32CMDAA","BROOKS","C"," ",{"$nulls":3}," "]
[74,"FI","10-0318","转子流量计","1110CK32CMDAA","BROOKS","C"," ",{"$nulls":3}," "]
[75,"TE","10-0319","热电阻","PR-24UBS-325MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[76,"TE","10-0320","热电阻","PR-24UBS-325MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[77,"PT","10-0321","差压变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[78,"FI","10-0323","转子流量计","1110CK31CMDAA","BROOKS","C"," ",{"$nulls":3}," "]
[81,"FT","10-0329","涡街","83F-A-01S1SSTNJ","FOXBORO US","C"," ",{"$nulls":3}," "]
[82,"TE","10-0330A","热电阻","PR-24UBS-40MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[83,"TE","10-0330B","热电阻","PR-24UBS-40MM","FOXBORO US","C"," ",{"$nulls":3}," "]
[85,"PI","10-0333","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[86,"PI","10-0334","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[87,"PI","10-0335","压力表","45-1279AS-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[88,"PI","10-0337","压力表","45-1279ASL-04L-XNH 1Mp","ASHCROFT","C"," ",{"$nulls":3}," "]
[89,"PI","10-0341","压力表","45-1279AS-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[90,"FT","10-0401","涡街","83F-A-01S1SSTNJ","FOXBORO US","C"," ",{"$nulls":3}," "]
[91,"FT","10-0402","涡街","83F-A-01S1SSTNJ","FOXBORO US","C"," ",{"$nulls":3}," "]
[92,"PI","10-0405","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[93,"FICV","10-0406","转子流量计","8800D3K2B1CA","BROOKS","C"," ",{"$nulls":3}," "]
[95,"PI","10-0409","压力表","45-1279ASL-04L-XNH 0-6Kg","ASHCROFT","C"," ",{"$nulls":3}," "]
[96,"FICV","10-0410","转子流量计","8800D3K2B1CA","BROOKS","C"," ",{"$nulls":3}," "]
[98,"PI","10-0413","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[99,"FICV","10-0414","转子流量计","8800D3K2B1CA","BROOKS","C"," ",{"$nulls":3}," "]
[101,"FICV","10-0416","转子流量计","8800D3K2B1CA","BROOKS","C"," ",{"$nulls":3}," "]
[103,"PI","10-0417","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[104,"PI","10-0419","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[105,"PI","10-0420","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[106,"PSL","10-0421","压力开关","PPDN7KKT06-XFSNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[109,"PI","10-0504","压力表","45-1279ASL-04L-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[110,"LT","10-0506","蒸发炉集液井液位变送器","1151LT4S",null,"C"," ",{"$nulls":3}," "]
[111,"PDI","10-0604","差压计","227","ITT BARTON","C"," ",{"$nulls":3}," "]
[112,"TE","10-0607","温包","45P-F5","FOXBORO US","C"," ",{"$nulls":3}," "]
[113,"FICV","10-0700","转子流量计","1350-8800","BROOKS","C"," ",{"$nulls":3}," "]
[115,"PI","10-0701","压力表","45-1279ASL-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[116,"FICV","10-0710","转子流量计","1350-8800","BROOKS","C"," ",{"$nulls":3}," "]
[118,"PI","10-0711","压力表","45-1279ASL-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[119,"FICV","10-0740","转子流量计","1350-8800","BROOKS","C"," ",{"$nulls":3}," "]
[121,"PI","10-0742","压力表","45-1279ASL-XNH","ASHCROFT","C"," ",{"$nulls":3}," "]
[122,"PI","10-1030","新丙酮卸料泵出口压","0~1MPa","青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[123,"PI","10-1031","新丙酮卸料泵出口压","0~1MPa","青岛四方仪表厂","C"," ",{"$nulls":3}," "]
[124,"PdI","10-2016","4#一级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[125,"TI","10-2017","4#一级VLA冷却器出口温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[126,"PI","10-2018","4#一级VLA冷却器出口压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[127,"TE","10-2021A","4#VLA风机10-205.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[128,"TT","10-2021A","4#VLA风机10-205.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[129,"TE","10-2021B","4#VLA风机10-205.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[130,"TT","10-2021B","4#VLA风机10-205.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[131,"TE","10-2022A","4#VLA风机10-205.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[132,"TT","10-2022A","4#VLA风机10-205.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[133,"TE","10-2022B","4#VLA风机10-205.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[134,"TT","10-2022B","4#VLA风机10-205.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[135,"TE","10-2022C","4#VLA风机10-205.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[136,"TT","10-2022C","4#VLA风机10-205.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[137,"TE","10-2023A","4#VLA风机10-205.00轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[138,"TT","10-2023A","4#VLA风机10-205.00轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[139,"TE","10-2023B","4#VLA风机10-205.00轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[140,"TT","10-2023B","4#VLA风机10-205.00轴承温度","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[141,"PdI","10-2027","4#二级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[142,"TT","10-2028","4#二级VLA冷却器温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[143,"PdI","10-2035","5#一级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[144,"TI","10-2036","5#一级VLA冷却器出口温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[145,"PI","10-2037","5#一级VLA冷却器出口压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[146,"TE","10-2040A","5#VLA风机10-206.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[147,"TT","10-2040A","5#VLA风机10-206.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[148,"TE","10-2040B","5#VLA风机10-206.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[149,"TT","10-2040B","5#VLA风机10-206.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[150,"TE","10-2041A","5#VLA风机10-206.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[151,"TT","10-2041A","5#VLA风机10-206.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[152,"TE","10-2041B","5#VLA风机10-206.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[153,"TT","10-2041B","5#VLA风机10-206.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[154,"TE","10-2041C","5#VLA风机10-206.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[155,"TT","10-2041C","5#VLA风机10-206.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[156,"TE","10-2042A","5#VLA风机10-206.00轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[157,"TT","10-2042A","5#VLA风机10-206.00轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[158,"TE","10-2042B","5#VLA风机10-206.00轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[159,"TT","10-2042B","5#VLA风机10-206.00轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[160,"PdI","10-2046","5#二级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[161,"TT","10-2047","5#二级VLA冷却器10-209.00出口温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[162,"TT","10-2049","二级冷却器出口总管温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[163,"PdI","10-2052","6#一级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[164,"TI","10-2053","6#一级VLA冷却器出口温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[165,"PI","10-2054","6#一级VLA冷却器出口压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[166,"TE","10-2057A","6#VLA风机10-207.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[167,"TT","10-2057A","6#VLA风机10-207.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[168,"TE","10-2057B","6#VLA风机10-207.00电机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[169,"TT","10-2057B","6#VLA风机10-207.00电机轴承温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[170,"TE","10-2058A","6#VLA风机10-207.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[171,"TT","10-2058A","6#VLA风机10-207.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[172,"TE","10-2058B","6#VLA风机10-207.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[173,"TT","10-2058B","6#VLA风机10-207.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[174,"TE","10-2058C","6#VLA风机10-207.00电机线圈温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[175,"TT","10-2058C","6#VLA风机10-207.00电机线圈温度变送器","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[176,"TE","10-2059A","6#VLA风机10-207.00轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[177,"TT","10-2059A","6#VLA风机10-207.00轴承温度","644RAI5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[178,"TE","10-2059B","6#VLA风机轴承温度热电阻","Pt100",null,"C"," ",{"$nulls":3}," "]
[179,"PdI","10-2063","6#二级VLA冷却器波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[180,"TT","10-2064","6#二级VLA冷却器一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[181,"FT","10-2102","6#VLA吸附床入口流量差压变送器","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[182,"FT","10-2110","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[183,"TT","10-2112","6#VLA吸附床温度温包温度变送器",null,"FOXBORO","C"," ",{"$nulls":3}," "]
[184,"TT","10-2113","6#VLA吸附床排出温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[185,"PT","10-2114","6#VLA吸附床压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[186,"LG","10-2115","6#VLA吸附床液位计",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[187,"PdI","10-2116","6#VLA吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[188,"FT","10-2118","7#VLA吸附床入口流量差压变送器","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[189,"FT","10-2126","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[190,"TT","10-2128","7#VLA吸附床温度温包温度变送器",null,"FOXBORO","C"," ",{"$nulls":3}," "]
[191,"TT","10-2129","7#VLA吸附床排出温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[192,"PT","10-2130","7#VLA吸附床压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[193,"LG","10-2131","7#VLA吸附床液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[194,"PdI","10-2132","7#VLA吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[195,"FT","10-2134","8#VLA吸附床入口流量差压变送器","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[196,"FT","10-2142","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[197,"TT","10-2144","8#VLA吸附床温度温包温度变送器",null,"FOXBORO","C"," ",{"$nulls":3}," "]
[198,"TT","10-2145","8#VLA吸附床排出温度",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[199,"PT","10-2146","8#VLA吸附床压力差压变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[200,"LG","10-2147","8#VLA吸附床液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[201,"PdI","10-2148","8#VLA吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[202,"TI","10-2151","5#吸附床冷凝器冷凝温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[203,"TT","10-2152","5#吸附床冷凝器冷凝温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[204,"TI","10-2154","6#吸附床冷凝器冷凝温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[205,"TT","10-2155","6#吸附床冷凝器冷凝温度",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[206,"TI","10-2157","4#吸附床冷凝器冷凝温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[207,"TT","10-2158","4#吸附床冷凝器冷凝温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[208,"FT","10-218","5#VLA吸附床入口流量","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[209,"FT","10-2201","9#VLA吸附床入口流量差压变送器","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[210,"FT","10-2209","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[211,"TT","10-2211","9#VLB吸附床温度温包温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[212,"TT","10-2212","9#VLB吸附床温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[213,"PT","10-2213","9#VLB吸附床压力压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[214,"LG","10-2214","9#VLB吸附床液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[215,"PdI","10-2215","9#VLB吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[216,"FT","10-2218","10#VLA吸附床入口流量差压变送器","3051SFADG360ZCHPS2T100031AA1A2RLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[217,"FT","10-2226","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[218,"TT","10-2228","10#VLA吸附床温度温包温度变送器",null,"FOXBORO","C"," ",{"$nulls":3}," "]
[219,"TT","10-2229","10#VLA吸附床排出温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[220,"PT","10-2230","10#VLA吸附床压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[221,"LG","10-2231","10#VLA吸附床液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[222,"PdI","10-2232","10#VLA吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[224,"LT","10-2237","吸附床排液盘2#收集槽液位液位变送器","3051S1LD2AA1A1010DFFJGDA00D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[225,"PI","10-2246","丙酮回收塔3#进料泵压力"," ","WIKA","C"," ",{"$nulls":3}," "]
[226,"FT","10-2250","进2#精馏塔稀丙酮流量涡街流量计","8800CW020SD3N1D1K5M5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[227,"FT","10-226","带温度补偿差压变送器","3095MFAS080ZCHPS1T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[228,"PI","10-2262","3#碱液进料泵压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[230,"TT","10-228","5#VLA吸附床温度温包温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[231,"TT","10-229","5#VLA吸附床排出温度一体化温度变送器","644HAI5XA/0065D02D0100D0500T44XA","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[232,"PT","10-230","5#VLA吸附床压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[233,"TT","10-2301","丙酮/水出4#丙酮回收塔进料预热器温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[234,"LG","10-2303","2#丙酮回收塔液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[235,"PI","10-2304","2#丙酮塔1# 残液泵压力表",null,"WIKA","C"," ",{"$nulls":3}," "]
[236,"PI","10-2305","2#丙酮塔进料预热器压力表",null,"WIKA","C"," ",{"$nulls":3}," "]
[237,"PI","10-2307","2#丙酮回收塔4#残液泵压力表",null,"WIKA","C"," ",{"$nulls":3}," "]
[238,"FI","10-2308","碱液至2#丙酮回收塔流量转子流量计",null,"科隆","C"," ",{"$nulls":3}," "]
[239,"LG","10-231","5#VLA吸附床液位",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[240,"TI","10-2310","2#丙酮塔进料预热器出口至碱贮槽温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[241,"LT","10-2311","2#丙酮回收塔液位变送器","3051S1LD2AA1A1010DFFJGDA00D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[242,"PT","10-2312","2#丙酮回收塔10-230.02底压力压力变送器","3051S2TG3A2B11A1AB4M5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[243,"TT","10-2313","2#丙酮回收塔底部温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[244,"TT","10-2314","2#丙酮回收塔13层板温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[245,"FI","10-2316","2#丙酮回收塔冷却水流量转子流量计",null,"科隆","C"," ",{"$nulls":3}," "]
[246,"FI","10-2318","2#2#丙酮回收塔冷却水流量转子流量计",null,"科隆","C"," ",{"$nulls":3}," "]
[247,"TT","10-2319","2#丙酮回收塔一体化温度变送器温度","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[248,"PdI","10-232","5#VLA吸附床蒸汽灭火系统波顿管差压计",null,"ITT","C"," ",{"$nulls":3}," "]
[249,"TT","10-2320","2#丙酮回收塔顶部温度一体化温度变送器","3144PD1A2I5B4M5Q4/0065D22D0035D0500T44","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[250,"PT","10-2321","2#丙酮回收塔顶层压力变送器","3051S1CD2A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[251,"FI","10-2323","2#丙酮回收塔去离子水流量转子流量计",null,"科隆","C"," ",{"$nulls":3}," "]
[252,"FT","10-2324","4#丙酮回收塔蒸汽流量差压变送器","3095MFAS060ZCHPS2T100T32CA1ARLM5Q4I5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[253,"PT","10-2326","蒸汽至2#丙酮回收塔压力变送器","3051S1TG2A2E11A1AB4D1I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[254,"LSHH","10-2327","2#丙酮回收塔回流罐液位开关",null,null,"C"," ",{"$nulls":3}," "]
[255,"LT","10-2328","丙酮回收塔回流罐液位单法兰液位变送器","3051S1LD2AA1A1020DFFJGDA00D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[256,"FT","10-2329","2#丙酮回收塔返回流量涡街流量计","8800CW010SD3N1D1K5M5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[257,"TT","10-2330A","2#丙酮回收塔顶冷凝器回流温度一体化温度变送器",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[258,"TT","10-2330B","2#丙酮回收塔顶冷凝器回流温度一体化温度变送器"," ","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[259,"LG","10-2331","2#MEO贮槽液位计",null,"ROSEMOUNT","C"," ",{"$nulls":3}," "]
[260,"LT","10-2332","2#MEO贮槽液位","3051S1LD2AA1A1020DFFJGDA00D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[261,"PI","10-2333","2#丙酮回收塔回流泵压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[262,"PI","10-2334","2#丙酮回收塔回流泵压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[263,"PI","10-2335","2#丙酮回收塔顶冷凝器压力指示"," ","WIKA","C"," ",{"$nulls":3}," "]
[264,"PI","10-2336","2#丙酮回收塔回流罐压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[265,"PI","10-2337","2#丙酮回收塔3#回流泵压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[266,"PI","10-2340","2#丙酮回收塔蒸汽压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[267,"PI","10-2341","2#丙酮塔进料预热器排放压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[268,"FT","10-2402","回收丙酮至3#,4#回收丙酮贮罐流量涡街流量计","8800CW010SD3N1D1K5M5","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[269,"PI","10-2405","3#回收丙酮贮罐压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[270,"LT","10-2406","3#回收丙酮贮罐液位变送器","3301HA1S1E5AM0300RAI5M1Q4","ROSEMOUNT","C"," ",{"$nulls":3}," ","比对"]
[271,"PI","10-2409","4#回收丙酮贮罐压力表"," ","WIKA","C"," ",{"$nulls":3}," "]
[272,"LT","10-2410","4#回收丙酮贮罐液位变送器","3301HA1S1E5AM0300RAI5M1Q4","ROSEMOUNT","C"," ",{"$nulls":3}," ","比对"]
[273,"TI","10-2603","丝束干燥排气温度双金属温度计",null,"ASHCROFT","C"," ",{"$nulls":3}," "]
[274,"PdT","10-2604","丝束干燥排气冷却机差压差压变送器","3051S1CD1A2E12A1AB4D1D2I5M5Q4","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[275,"TT","10-2607","丝束干燥排气冷却机温度一体化温度变送器","644HAI5M5XA/0065202D0100D0300T44XA","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[277,"FT","10-2015","至丙酮3KG蒸汽流量计      ","3095MFAS","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[278,"FT","17-0015","3KG蒸汽流量变送器        ","3095MFAS160Z","ROSEMOUNT","C"," ",{"$nulls":3}," "]
[279,"FT","17-0019","冷凝水回流至锅炉流量","YF104-ASS4J-S3S3*DNF1","上海横河","C"," ",{"$nulls":3}," "]
[280,"PI","17-0025","压力表          ","#45-1279AS          ","ASHCROFT","C"," ",{"$nulls":3}," "]
[281,"PI","17-0030","压力表          ","#45-1279AS          ","ASHCROFT","C"," ",{"$nulls":3}," "]
[282,"TE","17-0033","带套管双支铂电阻        ","PR-23UBS-006        ","FOXBORO US","C"," ",{"$nulls":3}," "]
[286,"TE","17-0102","带套管双支铂电阻        ","PR-23UBS-003        ","FOXBORO US","C"," ",{"$nulls":3}," "]
[294,"PSL","17-0603","压力开关","PPDN7KKT06","ASHCROFT","C"," ",{"$nulls":3}," "]
[295,"FT","17-0605","至喷丝帽清洗间丙酮流量","83F-A-01S1SSTNJ","FOXBORO ","C"," ",{"$nulls":3}," "]
[296,"PSL","17-0606","压力开关","PPDN7KKT06","ASHCROFT","C"," ",{"$nulls":3}," "]
[298,"FT","25-0743","电磁流量管","E83FA01S1STCDZ","FOXBORO ","C"," ",{"$nulls":3}," "]
[299,"LT","10-0252","稀碱制备贮槽液位",null,null,"C"]
[300,"LG","10-0115","1#吸咐床床底液位计",null,null,"C"]
[301,"LG","10-0131","2#吸咐床床底液位计",null,null,"C"]
[302,"LG","10-0147","3#吸咐床床底液位计",null,null,"C"]
[303,"LG","10-0214","4#吸咐床床底液位计",null,null,"C"]
[304,"LG","10-0303","1#回收塔液位计",null,null,"C"]
[305,"LG","10-0243","1#稀丙酮槽液位计",null,null,"C"]
[306,"LG","10-0245","2#稀丙酮槽液位计",null,null,"C"]
[307,"FT","10-2761","至丙酮回收氮气流量变送器",null,null,"C"]
[308,"FT","17-016","至丝束大楼3KG蒸汽流量","3095MFA","ROSEMOUNT","C"]
[310,"TI","10-3003","热水回收槽循环水回水双金属温度计","0~100℃","WIKA","C"]
[311,"TI","10-3004","热水回收槽送水双金属温度计","0~100℃","WIKA","C"]
[312,"PI","10-3005","热水回收槽送水压力表","Y100 0~1.6MPa","WIKA","C"]
[313,"TI","10-3006","热水回收槽循环水供水双金属温度计","0~100℃","WIKA","C"]
[314,"PI","10-3007","热水回收槽循环水供水压力表","Y100 0~1.6MPa","WIKA","C"]
[315,"PI","10-3009","压力表","Y100 0~1.6MPa","WIKA","C"]
[316,"TI","10-3008","7# VLA吸附床冷凝器出口丙酮双金属温度计","0~100℃","WIKA","C"]
[317,"LI","10-3001","热水回收槽液位计",null,null,"C"]
[318,"TT","10-801","1#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[319,"TT","10-802","2#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[320,"TT","10-809","3#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[321,"TT","10-810","4#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[322,"TT","10-803","5#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[323,"TT","10-804","6#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[324,"TT","10-805","界外1#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[325,"TT","10-806","界外2#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[326,"TT","10-807","1#稀丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[327,"TT","10-808","2#丙酮槽温度一体化温度变送器","0065传感器+644温变","ROSEMOUNT","C"]
[21,"TTE/MTE","-11-017-A","01",1,"一期纺丝一层风机出口温度湿度变送器","HMP3603","VAISALA"]
[22,"TTE/MTE","-11-018-A","01",1,"一期纺丝二层风机出口温度湿度变送器","HMP3603","VAISALA"]
[23,"TTE/MTE","-11-021-A","01",1,"一期干燥卷曲区风机出口温度湿度变送器","HMP3603","VAISALA"]
[24,"TTE/MTE","-11-217-A","01",1,"二期纺丝一层风机出口温度湿度变送器","HMP3603","VAISALA"]
[25,"TTE/MTE","-11-221-A","01",1,"二期干燥卷曲区风机出口温度湿度变送器","HMP3603","VAISALA"]
[29,"TTE/MTE","-11-214-A","01",1,"制浆一层风机出口温度湿度变送器","HMP3603","VAISALA"]
[30,"TTE/MTE","-11-014-A","01",1,"制浆二层风机出口温度湿度变送器","HMP3603","VAISALA"]
[31,"TTE/MTE","-11-218-A","02",2,"二期纺丝二层风机出口温度湿度变送器","HMP3603","VAISALA"]
[32,"DPT","-11-014-","01",1,"制浆二层室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[33,"DPT","-11-017-","01",1,"纺丝室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[34,"TTE","-11-034-","01",1,"MCC1室内温度变送器","644RAI5","ROSEMOUNT"]
[35,"DPT","-11-034-","01",1,"MCC1室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[36,"DPT","-11-036-","01",1,"喷丝帽清洗间室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[37,"TE","-11-052-","01",1,"纺丝一期I/O 机柜间温度温度变送器","644RAI5","ROSEMOUNT"]
[38,"TE","-11-052-","02",2,"MCC2室内温度温度变送器","644RAI5","ROSEMOUNT"]
[39,"TTE","-11-073-","01",1,"制浆I/O机柜间温度温度变送器","644RAI5","ROSEMOUNT"]
[40,"DPT","-11-214-","01",1,"制浆一层室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[41,"DPT","-11-223-","01",1,"二期摆丝室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[42,"DPT","-11-023-","01",1,"一期摆丝室内外差压变送器","3051S1CD0A2F12A1AB1D1D2K5L4M504","ROSEMOUNT"]
[43,"TT","-11-224-","01",1,"224-01排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[44,"TT","-11-224-","02",2,"224-02排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[45,"TT","-11-224-","03",3,"224-03排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[46,"TT","-11-224-","04",4,"224-04排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[47,"TE","-11-224-","05",5,"224-05排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[48,"TT","-11-224-","06",6,"224-06排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[49,"TT","-11-224-","07",7,"224-07排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[50,"TT","-11-224-","08",8,"224-08排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[51,"TT","-11-260-","01",1,"260-01排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[52,"TT","-11-260-","02",2,"260-02排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[53,"TT","-11-260-","03",3,"260-03排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[54,"TT","-11-260-","04",4,"260-04排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[55,"TT","-11-260-","05",5,"260-05排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[56,"TT","-11-260-","06",6,"260-06排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[57,"TT","-11-260-","07",7,"260-07排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[58,"TT","-11-260-","08",8,"260-08排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[59,"TT","-11-264-","01",1,"264-01排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[60,"TT","-11-264-","02",2,"264-02排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[61,"TT","-11-264-","03",3,"264-03排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[62,"TT","-11-264-","04",4,"264-04排风机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[63,"TT","-11-217-","01",1,"11-217电机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[64,"TT","-11-218-","01",1,"11-218电机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[65,"TT","-11-221-","01",1,"11-221电机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[66,"TT","-11-223-","01",1,"11-223电机温度变送器","644HAI5XAM5Q4  SENSOR:PT100.3WIRE","ROSEMOUNT"]
[67,"PI","-214-","01",1,"11-214空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[68,"PI","-214-","02",2,"11-214空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[69,"PI","-214-","03",3,"11-214空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[70,"PI","-214-","04",4,"11-214空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[71,"PI","-214-","05",5,"11-214空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[72,"PI","-214-","06",6,"11-214空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[73,"PI","-217-","01",1,"11-217空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[74,"PI","-217-","02",2,"11-217空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[75,"PI","-217-","03",3,"11-217空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[76,"PI","-217-","04",4,"11-217空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[77,"PI","-217-","05",5,"11-217空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[78,"PI","-217-","06",6,"11-217空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[79,"PI","-218-","01",1,"11-218空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[80,"PI","-218-","02",2,"11-218空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[81,"PI","-218-","03",3,"11-218空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[82,"PI","-218-","04",4,"11-218空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[83,"PI","-218-","05",5,"11-218空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[84,"PI","-218-","06",6,"11-218空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[85,"PI","-221-","01",1,"11-221空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[86,"PI","-221-","02",2,"11-221空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[87,"PI","-221-","03",3,"11-221空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[88,"PI","-221-","04",4,"11-221空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[89,"PI","-221-","05",5,"11-221空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[90,"PI","-221-","06",6,"11-221空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[91,"PI","-223-","01",1,"11-223空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[92,"PI","-223-","02",2,"11-223空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[93,"PI","-223-","03",3,"11-223空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[94,"PI","-223-","04",4,"11-223空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[95,"PI","-223-","05",5,"11-223空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[96,"PI","-223-","06",6,"11-223空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[97,"PI","-233-","01",1,"11-233空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[98,"PI","-233-","02",2,"11-233空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[99,"PI","-233-","03",3,"11-233空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[100,"PI","-233-","04",4,"11-233空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[101,"PI","-233-","05",5,"11-233空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[102,"PI","-233-","06",6,"11-233空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[103,"PI","-237-","01",1,"11-237空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[104,"PI","-237-","02",2,"11-237空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[105,"PI","-237-","03",3,"11-237空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[106,"PI","-237-","04",4,"11-237空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[107,"PI","-237-","05",5,"11-237空调蒸汽蒸汽压力表","0~0.6MPa","ASHCROFT"]
[108,"PI","-237-","06",6,"11-237空调蒸汽蒸汽压力表","0~0.6MPa","ASHCROFT"]
[109,"PI","-240-","01",1,"11-240空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[110,"PI","-240-","02",2,"11-240空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[111,"PI","-240-","03",3,"11-240空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[112,"PI","-240-","04",4,"11-240空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[113,"PI","-240-","05",5,"11-240空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[114,"PI","-240-","06",6,"11-240空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[115,"PI","-252-","01",1,"11-252空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[116,"PI","-252-","02",2,"11-252空调机组冷冻水压力表","0~0.4MPa","ASHCROFT"]
[117,"PI","-252-","03",3,"11-252空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[118,"PI","-252-","04",4,"11-252空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[119,"PI","-252-","05",5,"11-252空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[120,"PI","-252-","06",6,"11-253空调机组蒸汽压力表","0~0.6MPa","ASHCROFT"]
[121,"TI","-214-","01",1,"214机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[122,"TI","-214-","02",2,"214机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[123,"TI","-214-","03",3,"214机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[124,"TI","-214-","04",4,"214机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[125,"TI","-214-","05",5,"214机组出风口双金属温度计","0~50℃","ASHCROFT"]
[126,"TI","-217-","01",1,"217机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[127,"TI","-217-","02",2,"217机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[128,"TI","-217-","03",3,"217机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[129,"TI","-217-","04",4,"217机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[130,"TI","-217-","05",5,"217机组出风口双金属温度计","0~50℃","ASHCROFT"]
[131,"TI","-218-","01",1,"218机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[132,"TI","-218-","02",2,"218机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[133,"TI","-218-","03",3,"218机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[134,"TI","-218-","04",4,"218机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[135,"TI","-218-","05",5,"218机组出风口双金属温度计","0~50℃","ASHCROFT"]
[136,"TI","-221-","01",1,"221机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[137,"TI","-221-","02",2,"221机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[138,"TI","-221-","03",3,"221机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[139,"TI","-221-","04",4,"221机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[140,"TI","-221-","05",5,"221机组出风口双金属温度计","0~50℃","ASHCROFT"]
[141,"TI","-223-","01",1,"223机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[142,"TI","-223-","02",2,"223机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[143,"TI","-223-","03",3,"223机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[144,"TI","-223-","04",4,"223机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[145,"TI","-223-","05",5,"223机组出风口双金属温度计","0~50℃","ASHCROFT"]
[146,"TI","-233-","01",1,"233机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[147,"TI","-233-","02",2,"233机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[148,"TI","-233-","03",3,"233机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[149,"TI","-233-","04",4,"233机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[150,"TI","-233-","05",5,"233机组出风口双金属温度计","0~50℃","ASHCROFT"]
[151,"TI","-237-","01",1,"237机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[152,"TI","-237-","02",2,"237机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[153,"TI","-237-","03",3,"237机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[154,"TI","-237-","04",4,"237机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[155,"TI","-237-","05",5,"237机组出风口双金属温度计","0~50℃","ASHCROFT"]
[156,"TI","-240-","01",1,"240机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[157,"TI","-240-","02",2,"240机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[158,"TI","-240-","03",3,"240机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[159,"TI","-240-","04",4,"240机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[160,"TI","-240-","05",5,"240机组出风口双金属温度计","0~50℃","ASHCROFT"]
[161,"TI","-252-","01",1,"252机组冷冻供水总管双金属温度计","0~50℃","ASHCROFT"]
[162,"TI","-252-","02",2,"252机组冷冻回水总管双金属温度计","0~50℃","ASHCROFT"]
[163,"TI","-252-","03",3,"252机组表冷器前双金属温度计","0~50℃","ASHCROFT"]
[164,"TI","-252-","04",4,"252机组表冷器后双金属温度计","0~50℃","ASHCROFT"]
[165,"TI","-252-","05",5,"252机组出风口双金属温度计","0~50℃","ASHCROFT"]
[166,"DPI","-252-","05",1,"252机组进风段差压计","-10~700Pa","DWYER"]
[167,"DPI","-252-","05",2,"252机组出风段差压计","-10~700Pa","DWYER"]
[168,"FI","-252-","05",1,"252机组冷冻水转子流量计"]
[169,"DPI","-233-","05",1,"233机组进风段差压计","-10~700Pa","DWYER"]
[170,"DPI","-233-","05",2,"233机组出风段差压计","-10~700Pa","DWYER"]
[171,"FI","-233-","05",1,"233机组冷冻水转子流量计"]
[172,"DPI","-221-","05",1,"221机组进风段差压计","-10~700Pa","DWYER"]
[173,"DPI","-221-","05",2,"221机组出风段差压计","-10~700Pa","DWYER"]
[174,"FI","-221-","05",1,"221机组冷冻水转子流量计"]
[175,"DPI","-223-","05",1,"223机组进风段差压计","-10~700Pa","DWYER"]
[176,"DPI","-223-","05",2,"223机组出风段差压计","-10~700Pa","DWYER"]
[177,"FI","-223-","05",1,"223机组冷冻水转子流量计"]
[178,"DPI","-218-","05",1,"218机组进风段差压计","-10~700Pa","DWYER"]
[179,"DPI","-218-","05",2,"218机组出风段差压计","-10~700Pa","DWYER"]
[180,"FI","-218-","05",1,"218机组冷冻水转子流量计"]
[181,"DPI","-217-","05",1,"217机组进风段差压计","-10~700Pa","DWYER"]
[182,"DPI","-217-","05",2,"217机组出风段差压计","-10~700Pa","DWYER"]
[183,"FI","-217-","05",1,"217机组冷冻水转子流量计"]
[184,"DPI","-214-","05",1,"214机组进风段差压计","-10~700Pa","DWYER"]
[185,"DPI","-214-","05",2,"214机组出风段差压计","-10~700Pa","DWYER"]
[186,"FI","-214-","05",1,"214机组冷冻水转子流量计"]
[187,"DPI","-240-","05",1,"240机组进风段差压计","-10~700Pa","DWYER"]
[188,"DPI","-240-","05",2,"240机组出风段差压计","-10~700Pa","DWYER"]
[189,"FI","-240-","05",1,"240机组冷冻水转子流量计"]
[190,"DPI","-237-","05",1,"240机组进风段差压计","-10~700Pa","DWYER"]
[191,"DPI",-237,"05",2,"240机组出风段差压计","-10~700Pa","DWYER"]
[192,"FI","-237-","05",1,"240机组冷冻水转子流量计"]
[193,"DPI","-219-","05",1,"3#预热风机进风段差压计","-10~700Pa","DWYER"]
[194,"DPI","-219-","05",2,"3#预热风机出风段差压计","-10~700Pa","DWYER"]
[195,"DPI","-220-","05",1,"4#预热风机进风段差压计","-10~700Pa","DWYER"]
[196,"DPI","-220-","05",2,"4#预热风机出风段差压计","-10~700Pa","DWYER"]
[197,"DPI","-019-","05",1,"1#预热风机进风段差压计","-10~700Pa","DWYER"]
[198,"DPI","-020-","05",1,"2#预热风机进风段差压计","-10~700Pa","DWYER"]
[199,"DPI","-021-","05",1,"21机组进风段差压计","-10~700Pa","DWYER"]
[200,"FI","-021-","05",1,"21机组冷冻水转子流量计"]
[201,"DPI","-023-","05",1,"23机组进风段差压","-10~700Pa","DWYER"]
[202,"FI","-023-","05",1,"23机组冷冻水转子流量计"]
[203,"DPI","-017-","05",1,"17机组进风段差压计","-10~700Pa","DWYER"]
[204,"FI","-017-","05",1,"17机组冷冻水转子流量计"]
[205,"DPI","-018-","05",1,"18机组进风段差压计","-10~700Pa","DWYER"]
[206,"FI","-018-","05",1,"18机组冷冻水转子流量计"]
[207,"DPI","-014-","05",1,"14机组进风段差压计","-10~700Pa","DWYER"]
[208,"FI","-014-","05",1,"14机组冷冻水转子流量计"]

{"sheet":"标准器具2025","index":2,"n_rows":90,"n_cols":6,"rows_kept":90,"merged":[[0,0,0,5]]}
["标准器具送检清单（2025年）"]
["序号","名称","规格","编号","数量","备注"]
[1,"水银温度计","（0--50）℃",2017,1,"物化检"]
[2,"水银温度计","（0--100）℃",2015,1,"物化检"]
[3,"钢直尺","（0--300）mm",140531,1,"物化检"]
[4,"钢直尺","（0--300）mm","ARL96027",1,"物化检"]
[4,"专用砝码","6kg",null,1,"物化检"]
[5,"专用砝码","5磅",null,1,"物化检"]
[6,"专用砝码","3kg",null,1,"物化检"]
[8,"空盒气压表","DYM3","92-3396",1,"物化检"]
[9,"氧弹",null,"SD07190S3",1,"化水实验室"]
[10,"频闪仪(带充电器）",null,"RH114B004",1,"纺丝"]
[10,"频闪仪",null,"RH22C1835",1,"纺丝"]
[null,"频闪仪(带充电器）",null,"RH1902B001",1,"纺丝"]
[11,"静电测试仪","EX715","2020-0038",1,"制备"]
[11,"静电测试仪","EX715","2020-1076",1,"制备"]
[12,"电子式绝缘电阻表","FLUKE 1550C",3084024,1,"热动"]
[13,"复合式多气体检测仪","RD-4",18051767,1,"热动"]
[14,"复合式多气体检测仪","RD-1",18051767,1,"热动"]
[14,"外径千分尺","（50--75）mm",940358,1,"界内机修"]
[15,"刀口角尺","63mm","93/880642",1,"界内机修"]
[16,"百分表","（0--10）mm",311706,1,"界内机修"]
[17,"外径千分表","0-25mm",91531,1,"界内机修"]
[18,"外径千分表","25-50mm",91532,1,"界内机修"]
[19,"测振仪","GM63A","JL233235",1,"界内机修"]
[20,"工作用辐射温度计","62MAX","49112859WS",1,"界内机修"]
[21,"游标卡尺","0-3000mm",91503,1,"界内机修"]
[20,"接地电阻表","ZC-8",95021988,1,"电修"]
[21,"多功能现场校验仪 ","FLUKE754",2408054,1,"仪修"]
[22,"压力膜块","700PD5  (-100~200)kPa",83854505,1,"仪修"]
[23,"压力膜块","700P01  (0~2.5)kPa",2032104,1,"仪修"]
[24,"压力膜块","700PD3  (0~±34)kPa",94654301,1,"仪修"]
[25,"压力模块","700P06  (0~700)kPa",6310606,1,"仪修"]
[26,"压力膜块","700P27  (0~2000)kPa",89002714,1,"仪修"]
[27,"热电偶",null,1,1,"仪修"]
[28,"热电偶",null,"FLU80PK2A",1,"仪修"]
[29,"数字温湿度计","HTC-1",140531,1,"仪修"]
[30,"压力表",null,null,2,"仪修"]
[]
[1,"频闪仪","DT-315P",6310007,1,"纺丝"]
[2,"频闪仪",null,null,1,"纺丝"]
[3,"温湿度仪","HM40","R0610651",1,"纺丝"]
[4,"静电测试仪",430,"0001430007000272",1,"制备"]
[5,"氧弹",null,"SD10013S3",1,"化水实验室"]
[6,"水银温度计","（0--50）℃",2021,1,"物化检"]
[7,"水银温度计","（0--100）℃","0406",1,"物化检"]
[8,"钢直尺","（0--30）mm",null,1,"物化检"]
[9,"专用砝码","6kg",null,1,"物化检"]
[10,"专用砝码","5磅",null,1,"物化检"]
[11,"专用砝码","2.5磅",null,2,"物化检"]
[12,"百分表",null,"18.11001",1,"界内机修"]
[13,"百分表",null,406666,1,"界内机修"]
[14,"千分表","（0--1）mm",1040718,1,"界内机修"]
[15,"外径千分尺","(25--50)mm",354898,1,"界内机修"]
[16,"外径千分尺","(25--50)mm",43499,1,"界内机修"]
[17,"杠杆千分尺","(0--25)mm",41596,1,"界内机修"]
[18,"杠杆千分表","(0--100)mm","5K26032",1,"界内机修"]
[19,"杠杆千分表","(0--100)mm",90196,2,"界内机修"]
[20,"杠杆千分表","(0--100)mm",100612,2,"界内机修"]
[21,"外径千分尺","(0--25)mm",89810,1,"界内机修"]
[22,"刀口角尺",null,"JL17006409",1,"界内机修"]
[23,"外径千分尺",null,1269106,1,"界内机修"]
[24,"游标卡尺","(0--150)mm",6201051658,1,"界内机修"]
[25,"测振仪","GM63A",null,1,"界内机修"]
[26,"测温仪","MT4 MAX",28810365,1,"界内机修"]
[27,"条式水平仪","200mm",871258,1,"界内机修"]
[28,"外径千分尺","(0--50)mm",94101,1,"综合维修"]
[29,"外径千分尺","(25--50)mm",42982,1,"综合维修"]
[30,"外径千分尺","(50--75)mm","G4552",1,"综合维修"]
[31,"外径千分尺","(75--100)mm",969735,1,"综合维修"]
[32,"外径千分尺","(100--125)mm",44719,1,"综合维修"]
[33,"游标卡尺","(0--500)mm",null,1,"综合维修"]
[34,"游标卡尺","(0--300)mm",3201741123,1,"综合维修"]
[35,"游标卡尺","(0--300)mm","94/582122",1,"综合维修"]
[36,"深度游标卡尺","(0--300)mm",501762,1,"综合维修"]
[37,"水银温度计","0.01分度",2483,1,"仪修"]
[38,"水银温度计","0.1分度",489,1,"仪修"]
[39,"钢直尺","（0--1000）mm","01",1,"仪修"]
[40,"电子秒表","SJ9-1",8148,1,"仪修"]
[41,"数显千分尺","（0--25）mm","293-340",1,"仪修"]
[42,"数显表面温度计","905-T2",59927,1,"仪修"]
[43,"多功能现场校验仪","FLUKE754",2409013,1,"仪修"]
[44,"压力膜块","700PD3  ",94754303,1,"仪修"]
[45,"压力膜块","750P07",3935120,1,"仪修"]
[46,"压力膜块","700P27  ",89152702,1,"仪修"]
[47,"压力模块","700P08",6320805,1,"仪修"]
[48,"复合式多气体检测仪","BH-4",18119075,1,"热动"]
[49,"测温仪",null,"83CB8",1,"热动"]
[50,"测温仪",null,2989730402,1,"热动"]
[51,"温湿度计","TH-602F",null,8,"物资供应部"]

{"sheet":"热动器具2025","index":3,"n_rows":12,"n_cols":9,"rows_kept":12,"merged":[[0,0,0,7]]}
["热动生产部测量器具台账"]
["序号","工器具名称","数量","设备编号","规格型号","厂家","检验周期","放置地点","   检验单位"]
[1,"8#红外线测温仪",1,"83CB8","RAYRPM20L3U",null,12,"锅炉汽机中控室","云南省计量院"]
[2,"红外线测温仪",1,"83CB8","RAYRPM20L3U",null,12,"动力站","云南省计量院"]
[3,"复合式多气体检测仪RD-03",1,"B07X618191","BH-4A","河南省保时安电子科技有限公司",12,"备用（办公室）","方圆计量"]
[4,"复合式多气体检测仪RD-04",1,18119075,"BH-4A","河南省保时安电子科技有限公司",12,"动力站","方圆计量"]
[5,"便携式复合气体检测报警器RD-01",1,18051767,"BH-4A","河南省保时安电子科技有限公司",12,"锅炉汽机中控室","方圆计量"]
[6,"便携式复合气体检测报警器RD-02",1,"RD-02","BH-4A","河南省保时安电子科技有限公司",12,"锅炉汽机中控室"]
[7,"手持式智能超声波流量计",1,"DLZ(自编号）","TUF-2000H","北京韩泰科技发展有限公司",12,"备用（办公室）"]
[8,"台式电导率仪",1,11638150179,"HK-307","北京华科仪电力仪表研究所",12,"热动实验室"]
[9,"台式精密酸度计",1,10235150282,"HK-3C","北京华科仪电力仪表研究所",12,"热动实验室"]
[10,"多气体检测仪",1,"RDJC001","MSA10117530",null,12,"动力站","内部"]

{"sheet":"实验室器具2025","index":4,"n_rows":39,"n_cols":8,"rows_kept":39,"merged":[[0,0,0,5]]}
["实验室设备请检清单"]
["序号","摆放地点","设备名称  ","型号","序列号","厂家","检定周期"]
[1,"化检室  ","干燥恒温箱","FED240","09-16640","BINDER",12]
[2,"物检室  ","拉力仪",5943,"5943R8697","INSTRON",24]
[3,"物检室  ","拉力仪",5943,"5943R8698","INSTRON",24]
[4,"物检室  ","拉力仪","68SC-1","68SC1B27603","INSTRON",24]
[5,"物检室  ","拉力仪","68SC-1","68SC1B27604","INSTRON",24]
[6,"物检室  ","滤棒综合测试台","CQS6","/","CERULEAN",24]
[7,"化检室  ","密度仪","DMA 4500M",81569878," Anton Paar",24]
[8,"化检室  ","密度仪","DMA 4500M",83050749,"Anton Paar",24]
[9,"化检室  ","气相色谱仪","TRACE 1610",724020009,"Thermo",24]
[10,"化检室  ","气相色谱仪"," TRACE 1310",117100462,"Thermo",24]
[11,"化检室  ","气相色谱仪","TRACE GC Ultra",20084574,"Thermo",24]
[30,"化检室  ","气相色谱仪","TRACE GC Ultra",20084575,"Thermo",24]
[12,"物检室  ","色差仪","ULtraScan VIS",10062101,"Hunter Lab",24]
[13,"化检室  ","折光率仪","Abbemat 350",81633111,"Anton Paar",24]
[14,"化检室  ","电子天平       ","PB602",1114441091,"METTLER TOLEDO",12]
[15,"化检室  ","电子天平","AB204-S",1123200673,"METTLER TOLEDO",12]
[16,"化检室  ","电子天平","AG204",1114441000,"METTLER TOLEDO",12]
[17,"化检室  ","电子天平","FA2004",139,"上海天平仪器厂",12]
[18,"化检室  ","电子天平","PL2002-IC",1230170212,"METTLER TOLEDO",12]
[19,"化检室  ","电子天平       ","MS204TS/02","B948665085","METTLER TOLEDO",12]
[20,"物检室  ","电子天平","XS204",1128222829,"METTLER TOLEDO",12]
[21,"化水检验室 ","电子天平","XS205",1128010666,"METTLER TOLEDO",12]
[22,"化水检验室 ","托利多电子天平","PL3002-IC",1229210308,"METTLER TOLEDO",12]
[23,"物检室  ","竖式切丝器","非标","QZ-01(自编号)","云南沃特液压公司",12]
[24,"物检室  ","横式定时切丝器","非标","QZ-02(自编号)","南通醋酸纤维有限公司",12]
[25,"化水检验(煤分析室)","电子天平","PL2002",1232140435,"METTLER TOLEDO",12]
[26,"物检(综合库）","电子台秤","TCS-30","00285286FE","METTLER TOLEDO",12]
[27,"化水检验(煤分析室)","电子台秤","TCS-60","BKY19445","METTLER TOLEDO",12]
[28,"化检室  ","电子天平","XPR204","C429433212","METTLER TOLEDO",12]
[29,"物检室","单丝线密度检测仪","FAVIMAT+",51169,"德国TEXTECHNO公司",12]
[30,"物检室","吸阻标准压降棒","PD26058","388mm","CERULEAN",12,"只能送郑州烟草研究院检"]
[31,"物检室","吸阻标准压降棒","PD26059","200mm","CERULEAN",12,"只能送郑州烟草研究院检"]
[32,"物检室","吸阻标准压降棒","JPD13067",497,"CERULEAN",12,"只能送郑州烟草研究院检"]
[33,"物检室","容量瓶","100ml",null,null,1]
[34,"物检室","容量瓶","200ml",null,null,1]
[35,"物检室","秒表",null,"PC2000A",null,1]
[36,"物检室","马弗炉","M110",51010272,"thermo(赛默飞世尔)",1]